{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":6,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","DCC601A51"]
[]
[]
[]
[]
["","","","","","DCC601A51."]
["Leistungsaufnahme","kW","","","","0.015"]
["Maximale Anzahl der anschließbaren Innengeräte","","","","","32"]
["Maximale Anzahl der anschließbaren Außengeräte @","","","","","7"]
["Abmessungen","Maßeinheit","","Höhe","mm","136"]
["","","","Breite","mm","384"]
["","","","Tiefe","mm","92"]
["Kommunikation","DIII-NET","","Anzahl","","1"]
["","","","Bemerkung","","DIII-NET (F1F2)"]
["","Ethernet","","Anzahl","","1"]
["","Eingangsklemme","Digital","Anzahl","","4"]
["Umgebungstemperatur","Betrieb","","Min.","°C","-10"]
["","","","Max.","°C","50"]
["","Lagerung","","Min.","°C","-20"]
["","","","Max.","°C","60"]
["","Umgebungstemperatur-=-Relative Luftfeuchte <-=-%","","","%","85"]
["Stromversorgung","Frequenz","","","Hz","50/60"]
["Spannungsversorgung","Spannung","","","V","110–240 AC"]
["Hinweise","","","","","(1) - Inklusive der Leistungsaufnahme der WAGO-Stromversorgung, des CPU-Moduls und des E/A-Moduls"]
["","","","","","(2) - Die Abmessungen beinhalten die WAGO-Stromversorgung, die CPU-Module, das E/A-Modul und den erforderlichen Platz zwischen den verschiedenen Teilen."]
["","","","","","(3) - Abmessungen des Zubehör-Bildschirms: Höhe: 209mm, Breite: 123mm, Tiefe: 8,5mm"]