{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EGSQH-A9W"]
[]
[]
[]
[]
["","","","","","EGSQH10S18AA9W"]
["Schalldruckpegel","Nom.","","","dBA","32.0 (6)"]
["Kältemittel","GWP","","","","2,090"]
["","Füllmenge","","","kg","1.80"]
["","Typ","","","","R-410A"]
["Betriebsbereich","Installationsraum","","Min.","°C","5.00"]
["","","","Max.","°C","30.0"]
["","Heizen","Wasserseite","Max.","°C","60.0 (7), 65.0 (8)"]
["","","","Min.","°C","24 (7), 24 (8)"]
["","Soleseite","","Min.","°C","-5.00"]
["","","","Max.","°C","20.0"]
["","Warmwasser","Wasserseite","Max.","°C","55 (7), 60 (9)"]
["","","","Min.","°C","25 (7), 25 (9)"]
["Leistungsaufnahme","Nom.","","","kW","2.38 (1), 2.89 (2)"]
["Sound power level","Nom.","","","dBA","46.0"]
["COP","","","","","4.33 (1), 3.18 (2)"]
["Abmessungen","Maßeinheit","","Breite","mm","600"]
["","","","Tiefe","mm","728"]
["","","","Höhe","mm","1,730"]
["Gehäuse","Material","","","","Vorbeschichtetes Blech"]
["","Farbe","","","","Weiß"]
["Speicher","Wasservolumen","","","l","180"]
["","Korrosionsschutz","","","","Anode"]
["","Isolierung","","Wärmeverlust","kWh / 24 h","1.36 (4)"]
["Gewicht","Maßeinheit","","","kg","210"]
["Raumheizen","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","ηs (Saisonale Effizienz Raumheizen)","%","194"]
["","","","Saisonale Effizienzklasse Raumheizen","","A+++"]
["","","","SCOP","","5.06"]
["","Wasserauslass 55 °C für durchschnittliches Klima","Allgemein","Seasonal space heating eff. class","","A++"]
["","","","ηs (Saisonale Effizienz Raumheizen)","%","139"]
["","","","SCOP","","3.68"]
["Heizleistung","Nom.","","","kW","10.3 (1), 9.20 (2)"]
["","Min.","","","kW","3.11 (1), 2.47 (2)"]
["","Max.","","","kW","13.0 (1), 11.9 (2)"]
["Power supply","Phase","","","","3~"]
["","Bezeichnung","","","","9W"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","400"]
["Strom","Empfohlene Sicherungen","","","A","25"]
["Hinweise","","","","","(1) - ETK/AFK 0 °C/-3 °C – LWC 35 °C(dT = 5 °C)"]
["","","","","","(2) - ETK/AFK 0 °C/-3 °C – LWC 45 °C(dT = 5 °C)"]
["","","","","","(3) - mit 40 % Propylenglykol"]
["","","","","","(4) - Wärmeverlust gemäß EN12897"]
["","","","","","(5) - einschließlich Rohrleitungen + PWT+ Reserveheizung / ohne Ausdehnungsgefäß"]
["","","","","","(6) - Der Schalldruckpegel wird in einem Abstand von 1 m vom Gerät mit einem Mikrophon gemessen. Dies ist ein relativer Wert, der vom Abstand und von der Umgebungsakustik abhängt."]
["","","","","","(7) - Durch Wärmepumpe"]
["","","","","","(8) - Durch Wärmepumpe + Reserveheizer"]
["","","","","","(9) - Durch Reserveheizer"]