{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":8,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSH-D3"]
[]
[]
[]
[]
["","","","","","EHSH04P30DA3","EHSH08P50DA3","EHSH08P30DA3"]
["Gehäuse","Farbe","","","","Verkehrsweiß (RAL9016) / Eisengrau (RAL7011)","Verkehrsweiß (RAL9016) / Eisengrau (RAL7011)","Verkehrsweiß (RAL9016) / Eisengrau (RAL7011)"]
["","Material","","","","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen"]
["Abmessungen","Maßeinheit","","Höhe","mm","1891","1896","1891"]
["","","","Breite","mm","595","790","595"]
["","","","Tiefe","mm","615","790","615"]
["Gewicht","Maßeinheit","","","kg","73.0","93.0","73.0"]
["PED","Kategorie","","","","art. 3.3","art. 3.3","art. 3.3"]
["Kältemittel","Typ","","","","R-32","R-32","R-32"]
["","GWP","","","","675.0","675.0","675.0"]
["","Füllmenge","","","kg","1.50","1.50","1.50"]
["Schallleistungspegel","Nom.","","","dB(A)","39","39","39"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","18","18","18"]
["","","","Max.","°C","65","65","65"]
["","Kühlung","Umgebung","Min.","°CTK","10","10","10"]
["","","Wasserseite","Min.","°C","5","5","5"]
["","","","Max.","°C","22","22","22"]
["Stromversorgung","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","230","230","230"]
["Elektroheizung","Spannungsversorgung","","Bezeichnung","","3V / 9W","3V / 9W","3V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~","1~ / 3~"]
["","","","Frequenz","Hz","50","50","50"]
["Hinweise","","","","","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897"]
["","","","","","(2) - T KW = 10 °C / T WW = 40 °C / T SP = 50 °C","(2) - T KW = 10 °C / T WW = 40 °C / T SP = 50 °C","(2) - T KW = 10 °C / T WW = 40 °C / T SP = 50 °C"]
["","","","","","(3) - T KW = 10 °C / T WW = 40 °C / T SP = 60 °C","(3) - T KW = 10 °C / T WW = 40 °C / T SP = 60 °C","(3) - T KW = 10 °C / T WW = 40 °C / T SP = 60 °C"]
["","","","","","(4) - T KW = 10 °C / T WW = 40 °C / T SP = 65 °C","(4) - T KW = 10 °C / T WW = 40 °C / T SP = 65 °C","(4) - T KW = 10 °C / T WW = 40 °C / T SP = 65 °C"]
["","","","","","","(5) - Aufheizen des Speichers nur mit Wärmepumpe, kein Elektroheizer"]