{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHSHB-E"]
[]
[]
[]
[]
["","","","","","EHSHB04P30EF","EHSHB04P30EG","EHSHB08P30EF","EHSHB08P50EF","EHSHB08P30EG","EHSHB08P50EG"]
["Gehäuse","Farbe","","","","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)"]
["","Material","","","","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen"]
["Abmessungen","Maßeinheit","","Höhe","mm","1,892","1,891","1,892","1,905","1,891","1,910"]
["","","","Breite","mm","594","594","594","792","594","792"]
["","","","Tiefe","mm","644","644","644","812","644","817"]
["Gewicht","Maßeinheit","","","kg","79","80.0","79","110","80.0","104"]
["PED","Kategorie","","","","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3","Art 4.3"]
["Kältemittel","Typ","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","GWP","","","","675","675.0","675","675","675.0","675.0"]
["","Füllmenge","","","kg","1.5","1.50","1.5","1.5","1.50","1.50"]
["Schallleistungspegel","Schallleistungspegel-=-Nom.-=-dB(A)","","","dB(A)","39","39","39","39","39","39"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","18","18","18","18","18","18"]
["","","","Max.","°C","65","65","65","65","65","65"]
["","Kühlung","Umgebung","Min.","°C TK","10","10","10","10","10","10"]
["","","Wasserseite","Min.","°C","5","5","5","5","5","5"]
["","","","Max.","°C","22","22","22","22","22","22"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","230","230","230","230","230","230"]
["Hinweise","","","","","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897"]