{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":9,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E3V / ERGA-EV7"]
[]
[]
[]
[]
["","","","","","EHVX04S23EJ3V / ERGA04EAV37","EHVX04S18EA3V / ERGA04EAV37","EHVX04S18EJ3V / ERGA04EAV37","EHVX04S23EA3V / ERGA04EAV37"]
["Heizleistung","Nom.","","","kW","4.36, 4.60","4.36, 4.60","4.36, 4.60","4.36, 4.60"]
["Kühlleistung","Nom.","","","kW","4.86, 4.52","4.86, 4.52","4.86, 4.52","4.86, 4.52"]
["Leistungsaufnahme","Heizen","","Nom.","kW","0.830, 1.26","0.830, 1.26","0.830, 1.26","0.830, 1.26"]
["","Kühlung","","Nom.","kW","0.810, 1.36","0.810, 1.36","0.810, 1.36","0.810, 1.36"]
["","Leistungsaufnahme-=-Warmwasser von 10&nbsp;°C bis 50&nbsp;°C","","Leistungsaufnahme-=-Warmwasser von 10&nbsp;°C bis 50&nbsp;°C-=-Nom.-=-kWh","kWh","3.01","2.48","2.48","3.01"]
["Aufwärmzeit von 10&nbsp;°C bis 50&nbsp;°C-=-h","h","","","","1 h 40 min","1 h 28 min","1 h 28 min","1 h 40 min"]
["COP","","","","","5.23, 3.65","5.23, 3.65","5.23, 3.65","5.23, 3.65"]
["EER","","","","","5.98, 3.32","5.98, 3.32","5.98, 3.32","5.98, 3.32"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","XL","L","L","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A","A","A","A"]
["Raumheizen","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-SCOP","","3.29","3.29","3.29","3.29"]
["","","","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","A++","A++","A++","A++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","4.96","4.96","4.96","4.96"]
["","","","Saisonale Effizienzklasse Raumheizen","","A+++","A+++","A+++","A+++"]
["Hinweise","","","","","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)"]