{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":11,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHVX-E6VG / ERGA04-08EVA"]
[]
[]
[]
[]
["","","","","","EHVX04S18EA6VG / ERGA04EAV3A","EHVX04S23EA6VG / ERGA04EAV3A","EHVX08S18EA6VG / ERGA06EAV3A","EHVX08S23EA6VG / ERGA06EAV3A","EHVX08S18EA6VG / ERGA08EAV3A","EHVX08S23EA6VG / ERGA08EAV3A"]
["Heizleistung","Nom.","","","kW","4.3 (1), 4.6 (2)","4.3 (1), 4.6 (2)","6.0 (1), 5.9 (2)","6.0 (1), 5.9 (2)","7.5 (1), 7.8 (2)","7.5 (1), 7.8 (2)"]
["Kühlleistung","Nom.","","","kW","4.86 (1), 4.52 (2)","4.86 (1), 4.52 (2)","5.96 (1), 5.09 (2)","5.96 (1), 5.09 (2)","6.25 (1), 5.44 (2)","6.25 (1), 5.44 (2)"]
["Leistungsaufnahme","Heizen","","Nom.","kW","0.85 (1), 1.26 (2)","0.85 (1), 1.26 (2)","1.24 (1), 1.69 (2)","1.24 (1), 1.69 (2)","1.63 (1), 2.23 (2)","1.63 (1), 2.23 (2)"]
["","Kühlung","","Nom.","kW","0.81 (1), 1.36 (2)","0.81 (1), 1.36 (2)","1.06 (1), 1.55 (2)","1.06 (1), 1.55 (2)","1.16 (1), 1.73 (2)","1.16 (1), 1.73 (2)"]
["","Leistungsaufnahme-=-Warmwasser von 10&nbsp;°C bis 50&nbsp;°C","","Leistungsaufnahme-=-Warmwasser von 10&nbsp;°C bis 50&nbsp;°C-=-Nom.-=-kWh","kWh","2.48","3.01","2.48","3.01","2.48","3.01"]
["Aufwärmzeit von 10&nbsp;°C bis 50&nbsp;°C-=-h","h","","","","1 h 28 min","1 h 40 min","1 h 28 min","1 h 40 min","1 h 28 min","1 h 40 min"]
["COP","","","","","5.1 (1), 3.65 (2)","5.1 (1), 3.65 (2)","4.85 (1), 3.5 (2)","4.85 (1), 3.5 (2)","4.6 (1), 3.5 (2)","4.6 (1), 3.5 (2)"]
["EER","","","","","5.98 (1), 3.32 (2)","5.98 (1), 3.32 (2)","5.61 (1), 3.28 (2)","5.61 (1), 3.28 (2)","5.4 (1), 3.14 (2)","5.4 (1), 3.14 (2)"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","L","XL","L","XL","L","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A+","A+","A+","A+","A+","A+"]
["Raumheizen","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-SCOP","","3.29","3.29","3.27","3.27","3.3","3.3"]
["","","","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","A++","A++","A++","A++","A++","A++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","4.54","4.54","4.52","4.52","4.61","4.61"]
["","","","Saisonale Effizienzklasse Raumheizen","","A+++","A+++","A+++","A+++","A+++","A+++"]
["Hinweise","","","","","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)","(2) - Bedingung 2: Kühlen: Ta 35°C - LWE 7°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45°C (DT = 5°C)"]