{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":9,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV32 / EVLQ-CV3"]
[]
[]
[]
[]
["","","","","","EHYHBH05AAV32 / EVLQ05CAV3","EHYHBH05AFV32 / EVLQ05CAV3","EHYHBH08AAV32 / EVLQ08CAV3","EHYHBH08AFV32 / EVLQ08CAV3"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A"]
["COP","","","","","5.04 (1), 3.58 (2)","5.04, 3.58","4.45, 3.42","4.45, 3.42"]
["Heizleistung","Nom.","","","kW","4.40 (1), 4.03 (2)"]
["","Min.","","","kW","1.80 (1), 1.80 (2)"]
["","Max.","","","kW","5.12 (1), 4.90 (2)"]
["Leistungsaufnahme","Heizen","","Nom.","kW","0.870 (1), 1.13 (2)"]
["Hinweise","","","","","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Bedingung: Ta TK/FK 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Bedingung: Ta TK/FK 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Bedingung: Ta TK/FK 7°C/6°C - LWC 45°C (Dt=5°C)","(2) - Bedingung: Ta TK/FK 7°C/6°C - LWC 45°C (Dt=5°C)"]
["","","","","","(3) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(3) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass","(3) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass","(3) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(4) - Bedingung 2: Kühlen: Ta 35°C - LWE 7℃ (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 45℃ (DT = 5°C)","(4) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass","(4) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass","(4) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(5) - Tamb 35 °C – LWE 7 °C (dT = 5 °C), Gasbrennwertsystem-Bypass"]
["","","","","","(6) - Tamb 35 °C – LWE 18 °C (dT = 5 °C), Gasbrennwertsystem-Bypass"]
["","","","","","(7) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(8) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass"]
["Heizleistung","Min.","","","kW","","1.80, 1.80","1.80, 1.80","1.80, 1.80"]
["","Nom.","","","kW","","4.40, 4.03","7.40, 6.89","7.40, 6.89"]
["","Max.","","","kW","","5.12, 4.90","10.0, 9.53","10.0, 9.53"]
["Leistungsaufnahme","Heizen","","Nom.","kW","","0.870, 1.13","1.66, 2.01","1.66, 2.01"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","","XL","XL","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","","A","A","A"]
["Raumheizen","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-SCOP","","","3.28","3.24","3.24"]
["","","","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","","A++","A++","A++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","","4.50","4.25","4.25"]
["","","","Saisonale Effizienzklasse Raumheizen","","","A+++","A++","A++"]