{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":29,"n_cols":9,"rows_kept":29,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBH-AV32"]
[]
[]
[]
[]
["","","","","","EHYHBH05AFV32","EHYHBH05AAV32","EHYHBH08AFV32","EHYHBH08AAV32"]
["Gehäuse","Farbe","","","","Weiß","Weiß","Weiß","Weiß"]
["","Material","","","","Vorbeschichtetes Blech","Vorbeschichtetes Blech","Vorbeschichtetes Blech","Vorbeschichtetes Blech"]
["Abmessungen","Maßeinheit","","Höhe","mm","902","902","902","902"]
["","","","Breite","mm","450","450","450","450"]
["","","","Tiefe","mm","164","164","164","164"]
["Gewicht","Maßeinheit","","","kg","30.0","30.0","31.2","31.2"]
["PED","Kategorie","","","","Art. 3, § 3, Ausgenommen vom PED-Geltungsbereich aufgrund Artikel 1, Punkt 3.6, 97/23/EG","Art. 3, § 3, Ausgenommen vom PED-Geltungsbereich aufgrund Artikel 1, Punkt 3.6, 97/23/EG","Kategorie I","Kategorie I"]
["Wasserseitiger Wärmetauscher","Wasserdurchfluss","Heizen","Max.","l/min","23.0 (7)","23.0","23.5 (7)","23.5"]
["Schallleistungspegel","Nom.","","","dB(A)","42.0","42.0","42.0","42.0"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","25 (8)","25","25 (8)","25"]
["","","","Max.","°C","55 (8)","55","55 (8)","55"]
["Stromversorgung","Bezeichnung","","","","V3","V3","V3","V3"]
["","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","230","230","230","230"]
["Verdrahtungsanschlüsse","Für Anschluss an Bedienpult","","Anzahl","","2","2","2","2"]
["","","","Bemerkung","","0,75 mm² bis 1,25 mm² (max. Länge 500 m)","0,75 mm² bis 1,25 mm² (max. Länge 500 m)","0,75 mm² bis 1,25 mm² (max. Länge 500 m)","0,75 mm² bis 1,25 mm² (max. Länge 500 m)"]
["Hinweise","","","","","(1) - Nur für Innengerät","","(1) - Nur für Innengerät"]
["","","","","","(2) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass","","(2) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(3) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass","","(3) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(4) - Min. required","","(4) - Min. required"]
["","","","","","(5) - Boiler-Bypass","","(5) - Boiler-Bypass"]
["","","","","","(6) - Für Betriebsbereich von *HYHB* und *HYKOMB33AA; siehe Betriebsbereichszeichnung","","(6) - Für Betriebsbereich von *HYHB* und *HYKOMB33AA; siehe Betriebsbereichszeichnung"]