{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":6,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYHBX-AV3"]
[]
[]
[]
[]
["","","","","","EHYHBX08AFV3"]
["Gehäuse","Farbe","","","","Weiß"]
["","Material","","","","Vorbeschichtetes Blech"]
["Abmessungen","Maßeinheit","","Höhe","mm","902"]
["","","","Breite","mm","450"]
["","","","Tiefe","mm","164"]
["Gewicht","Maßeinheit","","","kg","31.2"]
["PED","Kategorie","","","","Kategorie I"]
["Wasserseitiger Wärmetauscher","Wasserdurchfluss","Heizen","Max.","l/min","23.5 (7)"]
["Schallleistungspegel","Nom.","","","dB(A)","42.0"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","25 (8)"]
["","","","Max.","°C","55 (8)"]
["","Kühlung","Umgebung","Min.","°CTK","10 (8)"]
["","","Wasserseite","Min.","°C","5 (8)"]
["","","","Max.","°C","22 (8)"]
["Stromversorgung","Bezeichnung","","","","V3"]
["","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["Spannungsversorgung","Spannung","","","V","230"]
["Verdrahtungsanschlüsse","Für Anschluss an Bedienpult","","Anzahl","","2"]
["","","","Bemerkung","","0,75 mm² bis 1,25 mm² (max. Länge 500 m)"]
["Hinweise","","","","","(1) - Nur für Innengerät"]
["","","","","","(2) - TK/FK 7 °C/6 °C – LWC 35 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(3) - TK/FK 7 °C/6 °C – LWC 45 °C(dT=5 °C), Boiler-Bypass"]
["","","","","","(4) - Tamb 35 °C – LWE 7 °C (dT = 5 °C), Gasbrennwertsystem-Bypass"]
["","","","","","(5) - Tamb 35 °C – LWE 18 °C (dT = 5 °C), Gasbrennwertsystem-Bypass"]
["","","","","","(6) - Min. required"]
["","","","","","(7) - Boiler-Bypass"]
["","","","","","(8) - Für Betriebsbereich von *HYHB* und *HYKOMB33AA; siehe Betriebsbereichszeichnung"]