{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":6,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EHYKOMB-AA3"]
[]
[]
[]
[]
["","","","","","EHYKOMB33AA3"]
["Gas","Anschluss","","Durchmesser","mm","15"]
["","Verbrauch (G20)","","Min.","m³/h","0.79"]
["","","","Max.","m³/h","3.39"]
["","Verbrauch (G25)","","Min.","m³/h","0.89"]
["","","","Max.","m³/h","3.92"]
["","Verbrauch (G31)","","Min.","m³/h","0.30"]
["","","","Max.","m³/h","1.29"]
["","NOx-klasse","","","","6"]
["","NOx-Niveau (G20)","","","mg/kWh","36"]
["Zentralheizung","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Min.","kW","7.6"]
["","","","Max.","kW","27.0"]
["","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","8.4"]
["","","","Max.","kW","30.0"]
["","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Min.-=-kW","kW","7.5"]
["","","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Nom.-=-kW","kW","26.6"]
["","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C","","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C-=-Nom.-=-kW","kW","8.2"]
["","Wassertemperatur","","Max.","°C","90"]
["Trinkwassererwärmung","Heizaufnahme (Netto-Brennwert) Qnw","Nom.","Min.","kW","7.6"]
["","","","Max.","kW","32.7"]
["","Heizaufnahme (Brutto-Brennwert) Qnw","Nom.","Min.","kW","8.4"]
["","","","Max.","kW","36.3"]
["","Komfortklassen (EN13203)","","","","XL"]
["","Temperatur","","Max.","°C","65"]
["Zufuhrluft","Konzentrisch","","","","Nein"]
["Rauchgas","Temperatur","","Max.","°C","70"]
["","Anschluss","","","mm","60"]
["","Massendurchfluss (G20)","","Max.","kg/h","54.4"]
["","Massendurchfluss (G25)","","Max.","kg/h","54.4"]
["","Massendurchfluss (G31)","","Max.","kg/h","53.6"]
["Gehäuse","Farbe","","","","RAL9010"]
["","Material","","","","Vorbeschichtetes Blech"]
["Abmessungen","Gerät","Höhe","Gehäuse","mm","710"]
["","Maßeinheit","","Breite","mm","450"]
["","","","Tiefe","mm","240"]
["Gewicht","Gerät","","Leer","kg","36"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","XL"]
["","","","Energieeffizienzklasse Wasserheizung","","A"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","A"]