{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EJHA-AV3"]
[]
[]
[]
[]
["","","","","","EJHA04AAV3"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","37.0"]
["Kältemittel","GWP","","","","675.0"]
["","Charge","","","kg","0.560"]
["","Typ","","","","R-32"]
["Betriebsbereich","Heizen","Umgebung","Max.","°C Feuchtkugel","25"]
["","Warmwasser","Umgebung","Min.","°C Trockenkugel","-14"]
["","","","Max.","°C Trockenkugel","35"]
["Leistungsaufnahme","Heizen","","Nom.","kW","0.850 (1)"]
["Schallleistungspegel","Heizen","","Nom.","dB(A)","58.7"]
["COP","","","","","4.49 (1)"]
["Abmessungen","Maßeinheit","","Breite","mm","845"]
["","","","Tiefe","mm","329"]
["","","","Höhe","mm","745"]
["Gewicht","Maßeinheit","","","kg","45.0"]
["Raumheizen","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","ηs (Saisonale Effizienz Raumheizen)","%","116"]
["","","","Saisonale Effizienzklasse Raumheizen","","A"]
["","","","SCOP","","2.98"]
["","Wasserauslass 55 °C für durchschnittliches Klima","Allgemein","Seasonal space heating eff. class","","A+"]
["","","","ηs (Saisonale Effizienz Raumheizen)","%","101"]
["","","","SCOP","","2.60"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","28.3"]
["Heizleistung","Nom.","","","kW","4.53 (1)"]
["Power supply","Phase","","","","1~"]
["","Bezeichnung","","","","V3"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","220-240"]
["Hinweise","","","","","(1) - Heizen: Wassertemp. Kondensatoraustritt 35°C, Dt 5 K; Umgebungstemp. 7°C Trockenkugel, 6°C Feuchtkugel"]