{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":78,"n_cols":7,"rows_kept":78,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHHE-PCV37"]
[]
[]
[]
[]
["","","","","","EKHHE200PCV37","EKHHE260PCV37"]
["Aufwärmzeit","Max.","","","hh:mm","06:27:00","09:29:00"]
["COP","","","","","3.23","3.37"]
["Trinkwassererwärmung","Abgabe","","Nom.","kW","1.339","1249"]
["Äquivalentes Warmwasser","Max.","","","l","241","335"]
["Abmessungen","Maßeinheit","","Höhe","mm","1607","1892"]
["","Gerät","","Durchmesser","mm","621","621"]
["Gewicht","Gerät","","Leer","kg","96","106"]
["","","","Voll","kg","283","353"]
["Abmessungen","Gerät","Höhe","Integriert in Innengerät","mm","1607","1892"]
["Gewicht","Versandpaket","","","kg","107","118"]
["Installationsort","","","","","Innen","Innen"]
["IP-klasse","","","","","IP24","IP24"]
["Verdichter","Typ","","","","Rollkolbenverdichter","Rollkolbenverdichter"]
["Kältemittel","Typ","","","","R-134a","R-134a"]
["Wärmepumpe","Bezeichnung","","","","EKHHE200PCV37","EKHHE260PCV37"]
["Kältemittel","GWP","","","","1430","1430"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","1.43","1.43"]
["","Füllmenge","","","kg","1","1"]
["Wärmepumpe","Heizleistung","","","kW","0.43","0.43"]
["","Gehäuse","","Farbe","","Weiß","Weiß"]
["","Abmessungen","Gerät","Höhe","mm","1607","1892"]
["","","","Breite","mm","621","621"]
["","","","Tiefe","mm","621","621"]
["","Gewicht","","Gerät","kg","96","106"]
["","","","Versandpaket","kg","107","118"]
["","Installationsort","","","","Nur Innengerät","Nur Innengerät"]
["","Installation","","IP-Klasse","","IP24","IP24"]
["","","","Abstand von der Wand","mm","200","200"]
["","Betriebsbereich","Umgebung","Min.","°C TK","-7","-7"]
["","","","Max.","°C TK","43","43"]
["","Schalldruckpegel","","Wärmepumpe-=-Schalldruckpegel-=-Nom.-=-dB(A)","dB(A)","53","51"]
["","","","Wärmepumpe-=-Schalldruckpegel-=-Nachteinstellungsmodus-=-dB(A)","dB(A)","53","51"]
["","Kältemittel","","Typ","","R-134A","R-134A"]
["","","","GWP","","1430","1430"]
["","","","Wärmepumpe-=-Kältemittel-=-Füllmenge-=-tCO2-Äq.","tCO2-Äq.","1.43","1.43"]
["","","","Füllmenge","kg","1","1"]
["","Abtauverfahren","","","","Heißgas-Abtauen","Heißgas-Abtauen"]
["","Systemdruck","","Max.","bar","7","7"]
["Speicher","Bezeichnung","","","","Speicher aus emailliertem Stahl - 200 Liter","Speicher aus emailliertem Stahl - 260 Liter"]
["","Leistung integriertes Heizelement","","Nom.","kW","1.5","1.5"]
["Trinkwassererwärmer","Gehäuse","","Farbe","","Weiß","Weiß"]
["","","","Material","","Emaillierter Stahl","Emaillierter Stahl"]
["","Installationsort","","","","Nur Innengerät","Nur Innengerät"]
["","Installation","","IP-Klasse","","IP24","IP24"]
["Speicher","Installation","","Solarwärmeanschluss möglich","","Ja","Ja"]
["Trinkwassererwärmer","Installation","","Rückstromöffnung Trinkwassererwärmer","","Nein","Nein"]
["Allgemein","Produktbeschreibung","","Luft-Wasser-Wärmepumpe","","Ja","Ja"]
["","","","Modellkennzeichnung","","EKHHE200PCV37","EKHHE260PCV37"]
["","Zusatzheizer","","Art der Energieaufnahme","","Elektroenergie","Elektroenergie"]
["","Lieferanten-/Herstellerdetails","","Name oder Marke","","Daikin Europe N.V.","Daikin Europe N.V."]
["","LW(A) Schallleistungspegel (entsprechend EN14825)","","Innen","dB(A)","53","51"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","L","XL"]
["","","","Funktion für feste Wasseraufheizung während Spitzenstunden","","Ja","Ja"]
["","","","Energieeffizienzklasse Wasserheizung","","A+","A+"]
["Warmwasserbereitung","Allgemein","","Thermostat-Temperatureinstellung","°C","55","55"]
["Schallleistungspegel","Warmwasserbereitung","","Schallleistungspegel-=-Warmwasserbereitung-=-Außengerät-=-dB(A)","dB(A)","45","44"]
["","","","Schallleistungspegel-=-Warmwasserbereitung-=-Innengerät-=-dB(A)","dB(A)","53","51"]
["Trinkwassererwärmung","Durchschnittliches Klima","","AEC (Jährlicher Stromverbrauch)","kWh","761","1210"]
["","","","Qelec (Täglicher Stromverbrauch)","kWh","2.08","3.31"]
["","Kaltes Klima","","AEC (Jährlicher Stromverbrauch)","kWh","944","1496"]
["","","","Qelec (Täglicher Stromverbrauch)","kWh","2.590","4.10"]
["","Warmes Klima","","AEC (Jährlicher Stromverbrauch)","kWh","631","1046"]
["","","","Qelec (Täglicher Stromverbrauch)","kWh","1.73","2.87"]
["Energieeffizienzbereich","","","","","A+ ~ F","A+ ~ F"]
["Wärmepumpe","Spannungsversorgung","","Phase","","1P","1P"]
["","","","Frequenz","Hz","50","50"]
["","","","Spannung","V","230","230"]
["","","","Maximaler Betriebsstrom","A","8.5","8.5"]
["","","","Empfohlene bauseitige Verwendung","A","2.43","2.43"]
["Speicher","Stromversorgung","","Phase","","1P","1P"]
["","","","Frequenz","Hz","50","50"]
["","","","Spannung","V","230","230"]