{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":7,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKHWET-BV3"]
[]
[]
[]
[]
["","","","","","EKHWET90BAV3","EKHWET120BAV3"]
["Montage","","","","","Wand","Wand"]
["Gehäuse","Farbe","","","","Weiß +Schwarz","Weiß +Schwarz"]
["","Material","","","","Blech, Acrylnitril-Butadien-Styrol","Blech, Acrylnitril-Butadien-Styrol"]
["Abmessungen","Gerät","Höhe","Speicher","mm","1032","1283"]
["","Maßeinheit","","Breite","mm","510","510"]
["","","","Tiefe","mm","570","570"]
["Gewicht","Gerät","","Leer","kg","43","47"]
["Trinkwassererwärmer","Wasservolumen","","","l","89","118"]
["","Material","","","","Emailbeschichteter Stahl DIN4753TL2","Emailbeschichteter Stahl DIN4753TL2"]
["Speicher","Maximale Wassertemperatur","","","°C","75.0","75.0"]
["Trinkwassererwärmer","Energieeffizienzklasse","","","","B","C"]
["Wärmetauscher","Trinkwassererwärmung","","Anzahl","","1","1"]
["","","","Rohrmaterial","","Aluminium","Aluminium"]
["","","","Betriebsdruck","bar","42","42"]
["Zusatzheizer","Leistung","","","kW","1.2","1.2"]