{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":71,"n_cols":11,"rows_kept":71,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EKOMBG-A"]
[]
[]
[]
[]
["","","","","","EKOMBG22AAV1","EKOMBG22ABV1","EKOMBG28AAV1","EKOMBG28ABV1","EKOMBG33AAV1","EKOMBG33ABV1"]
["Trinkwassererwärmung","Heizaufnahme (Brutto-Brennwert) Qnw","Nom.","Max.","kW","25.9","","23.3","","36.3"]
["","","","Min.","kW","6.1","","7.9","","8.4"]
["","Komfortklassen (EN13203)","","","","L","","XL","","XL"]
["","Temperatur","","Max.","°C","65","","65","","65"]
["","Heizaufnahme (Netto-Brennwert) Qnw","Nom.","Min.","kW","5.5","","7.1","","7.6"]
["","","","Max.","kW","23.3","","29.1","","32.7"]
["Rauchgas","Temperatur","","Max.","°C","70","","70","","70"]
["","Massendurchfluss (G31)","","Max.","kg/h","38.2","","47.9","","53.6"]
["Zufuhrluft","Konzentrisch","","","","60/100","","60/100","","60/100"]
["Trinkwassererwärmung","Allgemein","","Energieeffizienzklasse Wasserheizung","","A","","A","","A"]
["","","","Deklariertes Lastprofil","","L","","XL","","XL"]
["Abmessungen","Maßeinheit","Höhe","Gehäuse","mm","590","","650","","710"]
["Gehäuse","Material","","","","Vorbeschichtetes Blech","","Vorbeschichtetes Blech","","Vorbeschichtetes Blech"]
["","Farbe","","","","RAL9010","","RAL9010","","RAL9010"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","A","","A","","A"]
["","","","ηs (Saisonale Effizienz Raumheizen)","%","91","","92","","93"]
["Zentralheizung","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","6.1","","7.9","","8.4"]
["","","","Max.","kW","25.9","","32.3","","36.3"]
["","Wassertemperatur","","Max.","°C","90","","90","","90"]
["","Abgabe Pn bei 80/60°C","","Min.","kW","6.0","","7.6","","8.3"]
["","","","Nom.","kW","22.6","","28.2","","32.0"]
["","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Max.","kW","23.3","","29.1","","32.7"]
["","","","Min.","kW","5.5","","7.1","","7.6"]
["Gas","Anschluss","","Durchmesser","mm","15","","15","","15"]
["","Verbrauch (G31)","","Min.","m³/h","0.21","","0.29","","0.30"]
["","","","Max.","m³/h","0.94","","1.19","","1.29"]
["","NOx-klasse","","","","6","","6","","6"]
["","Anschluss","","Durchmesser","mm","","15","","15","","15"]
["","Verbrauch (G20)","","Min.","m³/h","","0.58","","0.74","","0.79"]
["","","","Max.","m³/h","","2.42","","3.02","","3.39"]
["","Verbrauch (G25)","","Min.","m³/h","","0.62","","0.84","","0.89"]
["","","","Max.","m³/h","","2.82","","3.46","","3.92"]
["","Verbrauch (G31)","","Min.","m³/h","","0.21","","0.29","","0.30"]
["","","","Max.","m³/h","","0.94","","1.19","","1.29"]
["","NOx-klasse","","","","","6","","6","","6"]
["","NOx-Niveau (G20)","","","mg/kWh","","28","","27","","36"]
["Zentralheizung","Heizaufnahme Qn (Netto-Brennwert)","Nom.","Min.","kW","","5.5","","7.1","","7.6"]
["","","","Max.","kW","","23.3","","29.1","","32.7"]
["","Heizaufnahme Qn (Brutto-Brennwert)","Nom.","Min.","kW","","6.1","","7.9","","8.4"]
["","","","Max.","kW","","25.9","","32.3","","36.3"]
["","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Min.-=-kW","kW","","6.0","","7.6","","8.3"]
["","","","Zentralheizung-=-Abgabe Pn bei 80/60&nbsp;°C-=-Nom.-=-kW","kW","","22.6","","28.2","","32.0"]
["","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C","","Zentralheizung-=-Abgabe bei 37/30&nbsp;°C-=-Nom.-=-kW","kW","","6.0","","7.6","","8.3"]
["","Wassertemperatur","","Max.","°C","","90","","90","","90"]
["Trinkwassererwärmung","Heizaufnahme (Netto-Brennwert) Qnw","Nom.","Min.","kW","","5.5","","7.1","","7.6"]
["","","","Max.","kW","","23.3","","29.1","","32.7"]
["","Heizaufnahme (Brutto-Brennwert) Qnw","Nom.","Min.","kW","","6.1","","7.9","","8.4"]
["","","","Max.","kW","","25.9","","23.3","","36.3"]
["","Komfortklassen (EN13203)","","","","","L","","XL","","XL"]
["","Temperatur","","Max.","°C","","65","","65","","65"]
["Zufuhrluft","Konzentrisch","","","","","Nein","","Nein","","Nein"]
["Rauchgas","Temperatur","","Max.","°C","","70","","70","","70"]
["","Anschluss","","","mm","","60","","60","","60"]
["","Massendurchfluss (G20)","","Max.","kg/h","","38.9","","48.6","","54.4"]
["","Massendurchfluss (G25)","","Max.","kg/h","","38.9","","48.6","","54.4"]
["","Massendurchfluss (G31)","","Max.","kg/h","","38.2","","47.9","","53.6"]
["Gehäuse","Farbe","","","","","RAL9010","","RAL9010","","RAL9010"]
["","Material","","","","","Vorbeschichtetes Blech","","Vorbeschichtetes Blech","","Vorbeschichtetes Blech"]
["Abmessungen","Gerät","Höhe","Gehäuse","mm","","590","","650","","710"]
["","Maßeinheit","","Breite","mm","","450","","450","","450"]
["","","","Tiefe","mm","","240","","240","","240"]
["Gewicht","Gerät","","Leer","kg","","30","","33","","36"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","","L","","XL","","XL"]
["","","","Energieeffizienzklasse Wasserheizung","","","A","","A","","A"]
["Raumheizen","Allgemein","","Saisonale Effizienzklasse Raumheizen","","","A","","A","","A"]