{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK06-10AV3"]
[]
[]
[]
[]
["","","","","","EPSK06ARV3","EPSK08ARV3","EPSK10ARV3"]
["Abmessungen","Maßeinheit","","Höhe","mm","1123","1123","1123"]
["","","","Breite","mm","1330","1330","1330"]
["","","","Tiefe","mm","604","604","604"]
["Gewicht","Maßeinheit","","","kg","174","174","174"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","75.7","75.7","75.7"]
["","","Kühlung","Hoch","m³/min","75.7","75.7","75.7"]
["Betriebsbereich","Kühlung","","Betriebsbereich-=-Kühlung-=-Min.-=-°C TK","°C TK","10","10","10"]
["","","","Betriebsbereich-=-Kühlung-=-Max.-=-°C TK","°C TK","43","43","43"]
["","Warmwasser","","Min.","°C TK","-28","-28","-28"]
["","","","Betriebsbereich-=-Warmwasser-=-Max.-=-°C TK","°C TK","40","40","40"]
["Schallleistungspegel","Heizen","","Nom.","dB(A)","45 (1)","45 (1)","47 (1)"]
["","Kühlung","","Nom.","dB(A)","52.2 (2)","53 (2)","53.2 (2)"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","32.6 (1)","32.4 (1)","32.8 (1)"]
["","Kühlung","","Nom.","dB(A)","36.9 (2)","37.2 (2)","37.3 (2)"]
["Kältemittel","Typ","","","","R-290","R-290","R-290"]
["","GWP","","","","3","3","3"]
["","Kältemittel-=-Füllmenge-=-tCO2-Äq.","","","tCO2-Äq.","0.003","0.003","0.003"]
["","Füllmenge","","","kg","1","1","1"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","m","10","10","10"]
["Stromversorgung","Bezeichnung","","","","V3","V3","V3"]
["","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50"]
["Spannungsversorgung","Spannung","","","V","230","230","230"]
["Strom","Empfohlene Sicherungen","","","A","25","25","25"]
["Hinweise","","","","","(1) - Gemessen bei LWC 47–55 °C; Ta TK/FK 7 °C/6 °C","(1) - Gemessen bei LWC 47–55 °C; Ta TK/FK 7 °C/6 °C","(1) - Gemessen bei LWC 47–55 °C; Ta TK/FK 7 °C/6 °C"]
["","","","","","(2) - Gemessen bei LWC 12–7 °C; Ta 35°C","(2) - Gemessen bei LWC 12–7 °C; Ta 35°C","(2) - Gemessen bei LWC 12–7 °C; Ta 35°C"]
["","","","","","(3) - 1 1/4\" Bauseitige Rohrleitungen","(3) - 1 1/4\" Bauseitige Rohrleitungen","(3) - 1 1/4\" Bauseitige Rohrleitungen"]
["","","","","","(4) - 1 1/2\" Bauseitige Rohrleitungen","(4) - 1 1/2\" Bauseitige Rohrleitungen","(4) - 1 1/2\" Bauseitige Rohrleitungen"]