{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":7,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSK12-14AW1"]
[]
[]
[]
[]
["","","","","","EPSK12ARW1","EPSK14ARW1"]
["Abmessungen","Maßeinheit","","Höhe","mm","1,123","1,123"]
["","","","Breite","mm","1,330","1,330"]
["","","","Tiefe","mm","604","604"]
["Gewicht","Maßeinheit","","","kg","191","191"]
["Ventilator","Luftstromvolumen","Heizen","Hoch","m³/min","96.3","96.3"]
["","","Kühlung","Hoch","m³/min","96.3","96.3"]
["Betriebsbereich","Kühlung","","Betriebsbereich-=-Kühlung-=-Min.-=-°C&nbsp;TK","°CTK","10","10"]
["","","","Betriebsbereich-=-Kühlung-=-Max.-=-°C&nbsp;TK","°CTK","43","43"]
["","Warmwasser","","Min.","°CTK","-28","-28"]
["","","","Betriebsbereich-=-Warmwasser-=-Max.-=-°C&nbsp;TK","°CTK","40","40"]
["Schallleistungspegel","Heizen","","Nom.","dB(A)","52 (1)","52 (1)"]
["","Kühlung","","Nom.","dB(A)","62 (2)","63 (2)"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","38 (1)","38 (1)"]
["","Kühlung","","Nom.","dB(A)","47 (2)","48 (2)"]
["Kältemittel","Typ","","","","R-290","R-290"]
["","GWP","","","","3","3"]
["","Füllmenge","","","tCO2Eq","0.0038","0.0038"]
["","Füllmenge","","","kg","1.25","1.25"]
["Rohrleitungsanschlüsse","Niveauunterschied","IG - AG","Max.","m","10","10"]
["Stromversorgung","Bezeichnung","","","","W1","W1"]
["","Phase","","","","3~","3~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","400","400"]
["Strom","Empfohlene Sicherungen","","","A","16","16"]
["Hinweise","","","","","(1) - Gemessen bei LWC 47–55 °C; Ta TK/FK 7 °C/6 °C","(1) - Gemessen bei LWC 47–55 °C; Ta TK/FK 7 °C/6 °C"]
["","","","","","(2) - Gemessen bei LWC 12–7 °C; Ta 35°C","(2) - Gemessen bei LWC 12–7 °C; Ta 35°C"]
["","","","","","(3) - 1 1/4\" Bauseitige Rohrleitungen","(3) - 1 1/4\" Bauseitige Rohrleitungen"]
["","","","","","(4) - 1 1/2\" Bauseitige Rohrleitungen","(4) - 1 1/2\" Bauseitige Rohrleitungen"]