{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":9,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","EPSX10A / EPSK08-10AW1"]
[]
[]
[]
[]
["","","","","","EPSX10P30AF / EPSK08ARW1","EPSX10P50AF / EPSK08ARW1","EPSX10P30AF / EPSK10ARW1","EPSX10P50AF / EPSK10ARW1"]
["Innengerät","","","","","EPSX10P30AF","EPSX10P50AF","EPSX10P30AF","EPSX10P50AF"]
["Heizleistung","Nom.","","","kW","7.62 (1)","7.62 (1)","8.11 (1)","8.11 (1)"]
["Kühlleistung","Nom.","","","kW","6.89 (2), 6.37 (3)","6.89 (2), 6.37 (3)","7.84 (2), 6.37 (3)","7.84 (2), 6.37 (3)"]
["Leistungsaufnahme","Heizen","","Nom.","kW","1.52 (1)","1.52 (1)","1.64 (1)","1.64 (1)"]
["","Kühlung","","Nom.","kW","1.85 (2), 1.13 (3)","1.85 (2), 1.13 (3)","2.17 (2), 1.13 (3)","2.17 (2), 1.13 (3)"]
["","Leistungsaufnahme-=-Warmwasser von 10 °C bis 50 °C","","Leistungsaufnahme-=-Warmwasser von 10 °C bis 50 °C-=-Nom.-=-kWh","kWh","3.42","5.25","3.42","5.25"]
["Aufwärmzeit von 10°C bis 50°C","h","","","","2h 21min","3h 34min","2h 21min","3h 34min"]
["COP","","","","","5.01 (1)","5.01 (1)","4.94 (1)","4.94 (1)"]
["EER","","","","","3.73 (2), 5.63 (3)","3.73 (2), 5.63 (3)","3.62 (2), 5.63 (3)","3.62 (2), 5.63 (3)"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","L","XL","L","XL"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A","A+","A","A+"]
["Raumheizen","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein-=-SCOP","","3.94","3.94","3.99","3.99"]
["","","","Raumheizen-=-Wasserauslass 55 °C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","A+++","A+++","A+++","A+++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","5.14","5.14","5.14","5.14"]
["","","","Saisonale Effizienzklasse Raumheizen","","A+++","A+++","A+++","A+++"]
["Energy Efficiency Range","","","","","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F","Space Heating A+++ ~ D, Water Heating A+ ~ F"]
["Hinweise","","","","","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - Kühlen: EW 12 °C; AW 7 °C; Umgebungsbedingungen: 35 °C TK","(2) - Kühlen: EW 12 °C; AW 7 °C; Umgebungsbedingungen: 35 °C TK","(2) - Kühlen: EW 12 °C; AW 7 °C; Umgebungsbedingungen: 35 °C TK","(2) - Kühlen: EW 12 °C; AW 7 °C; Umgebungsbedingungen: 35 °C TK"]
["","","","","","(3) - Kühlen: EW 23 °C; AW 18 °C; Umgebungsbedingungen: 35 °C TK","(3) - Kühlen: EW 23 °C; AW 18 °C; Umgebungsbedingungen: 35 °C TK","(3) - Kühlen: EW 23 °C; AW 18 °C; Umgebungsbedingungen: 35 °C TK","(3) - Kühlen: EW 23 °C; AW 18 °C; Umgebungsbedingungen: 35 °C TK"]