{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":60,"n_cols":8,"rows_kept":60,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERSQ-AV1"]
[]
[]
[]
[]
["","","","","","ERSQ011AAV1","ERSQ014AAV1","ERSQ016AAV1"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","","53"]
["Standardzubehör","Installationsanleitung","","","","","1"]
["Kältemittel","GWP","","","","","2,087.5"]
["","Füllmenge","","","kg","","4.5"]
["","Typ","","","","","R-410A"]
["Betriebsbereich","Heizen","","Max.","°C FK","","20"]
["","","","Min.","°C FK","","-20"]
["","Warmwasser","","Min.","°CTK","","-20"]
["","","","Max.","°CTK","","35"]
["Rohrleitungsanschlüsse","Wärmeisolierung","","","","","Sowohl Flüssigkeits- als auch Gasleitungen"]
["","Flüssigkeit","","AD","mm","","9.52"]
["","Gas","","AD","mm","","15.9"]
["","Ableitung","","AD","mm","","26x3"]
["","Niveauunterschied","IG - AG","Max.","m","","30"]
["Sound power level","Heating","","Nom.","dB(A)","","69"]
["Abmessungen","Maßeinheit","","Breite","mm","","900"]
["","","","Tiefe","mm","","320"]
["","","","Höhe","mm","","1,345"]
["Gewicht","Maßeinheit","","","kg","","120"]
["Power supply","Phase","","","","","1~"]
["","Bezeichnung","","","","","V1"]
["","Frequenz","","","Hz","","50"]
["","Spannung","","","V","","220-440"]
["Strom","Empfohlene Sicherungen","","","A","","25"]
["Hinweise","","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","(2) - Zmax: Möglicherweise müssen Sie gemäß EN/IEC 61000-3-11 sich an den Vertriebsnetzmitarbeiter wenden, um sicherzustellen, dass die Anlage nur an eine Versorgung mit Zsys (Systemimpedanz) ≤ Zmax angeschlossen wird."]
["","","","","","","(3) - EN/IEC 61000-3-11: Europäisches/internationales Regelwerk bezüglich Grenzwerte: Begrenzung von Spannungsänderungen, Spannungsschwankungen und Flickern in öffentlichen Niederspannungs-Versorgungsnetzen; Geräte und Einrichtungen mit Bemessungsströmen ≤ 75 A."]
["","","","","","","(4) - Min. Ssc-Wert (Kurzschluss-Strom): Anlage entspricht Forderungen der EN/IEC 61000-3-12: Europanorm / internat. Norm zur Festlegung der Grenzwerte für Oberschwingungsströme, verursacht von Geräten / Einrichtungen mit Eingangsstrom > 16 A und ≤ 75 A je Leiter, die zum Anschluss an öffentliche Niederspannungsnetze vorgesehen sind"]
["","","","","","","(5) - Enthält fluorierte Treibhausgase"]
["Abmessungen","Maßeinheit","","Höhe","mm","1345","","1345"]
["","","","Breite","mm","900","","900"]
["","","","Tiefe","mm","320","","320"]
["Gewicht","Maßeinheit","","","kg","120","","120"]
["Betriebsbereich","Heizen","","Min.","°C FK","-20","","-20"]
["","","","Max.","°C FK","20","","20"]
["","Warmwasser","","Min.","°CTK","-20","","-20"]
["","","","Betriebsbereich-=-Warmwasser-=-Max.-=-°C&nbsp;TK","°CTK","35","","35"]
["Schallleistungspegel","Heizen","","Nom.","dB(A)","68","","71"]
["Schalldruckpegel","Heizen","","Schalldruckpegel-=-Heizen-=-Nom.-=-dBA","dB(A)","52","","55"]
["Kältemittel","Typ","","","","R-410A","","R-410A"]
["","GWP","","","","2087.5","","2087.5"]
["","Füllmenge","","","tCO2Eq","9.4","","9.4"]
["","Füllmenge","","","kg","4.5","","4.5"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","","9.52"]
["","Gas","","AD","mm","15.9","","15.9"]
["","Ableitung","","AD","mm","26x3","","26x3"]
["","Niveauunterschied","IG - AG","Max.","m","30","","30"]
["","Wärmeisolierung","","","","Sowohl Flüssigkeits- als auch Gasleitungen","","Sowohl Flüssigkeits- als auch Gasleitungen"]
["Standardzubehör","Installation manual","","","","1","","1"]
["Stromversorgung","Bezeichnung","","","","V1","","V1"]
["","Phase","","","","1~","","1~"]
["","Frequenz","","","Hz","50","","50"]
["Spannungsversorgung","Spannung","","","V","220-440","","220-440"]
["Strom","Empfohlene Sicherungen","","","A","25","","25"]