{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ERWQ-AV3"]
[]
[]
[]
[]
["","","","","","ERWQ02AAV3"]
["Abmessungen","Maßeinheit","","Höhe","mm","550"]
["","","","Breite","mm","765"]
["","","","Tiefe","mm","285"]
["Gewicht","Maßeinheit","","","kg","35"]
["Betriebsbereich","Warmwasser","","Max.","°CTK","35"]
["","","","Min.","°CTK","-15"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35"]
["","Gas","","AD","mm","9.5"]
["","Niveauunterschied","IG - AG","Max.","m","15"]
["Schalldruckpegel","Heizen","","Nom.","dB(A)","47"]
["","Kühlung","","Nom.","dB(A)","47"]
["Kältemittel","Typ","","","","R-410A"]
["","GWP","","","","2,087.5"]
["","Füllmenge","","","kg","1.05"]
["Power supply","Bezeichnung","","","","V3"]
["","Phase","","","","1~"]
["","Frequenz","","","Hz","50"]
["","Spannung","","","V","230"]
["Hinweise","","","","","(1) - Enthält fluorierte Treibhausgase"]