{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":17,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH12E / EPRA08-12EW"]
[]
[]
[]
[]
["","","","","","ETSH12P30EF / EPRA08EAW1","ETSH12P50EF / EPRA08EAW1","ETSH12P30EG / EPRA08EAW1","ETSH12P50EG / EPRA08EAW1","ETSH12P30EF / EPRA10EAW1","ETSH12P50EF / EPRA10EAW1","ETSH12P50EG / EPRA10EAW1","ETSH12P30EG / EPRA10EAW1","ETSH12P30EF / EPRA12EAW1","ETSH12P50EF / EPRA12EAW1","ETSH12P50EG / EPRA12EAW1","ETSH12P30EG / EPRA12EAW1"]
["Innengerät","","","","","ETSH12P30EF","ETSH12P50EF","ETSH12P30EG","ETSH12P50EG","ETSH12P30EF","ETSH12P50EF","ETSH12P50EG","ETSH12P30EG","ETSH12P30EF","ETSH12P50EF","ETSH12P50EG","ETSH12P30EG"]
["Heizleistung","Nom.","","","kW","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)","6.17 (1)"]
["Leistungsaufnahme","Heizen","","Nom.","kW","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)","1.21 (1)"]
["COP","","","","","5.1","5.1","5.10 (1)","5.10 (1)","5.1","5.1","5.10 (1)","5.10 (1)","5.1","5.1","5.10 (1)","5.10 (1)"]
["Trinkwassererwärmung","Allgemein","","Deklariertes Lastprofil","","L","XL","L","XL","L","XL","XL","L","L","XL","XL","L"]
["","Durchschnittliches Klima","","Energieeffizienzklasse Wasserheizung","","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+","A+"]
["Raumheizen","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-SCOP","","3.52","3.52","3.52","3.52","3.53","3.53","3.53","3.53","3.53","3.53","3.53","3.53"]
["","","","Raumheizen-=-Wasserauslass 55&nbsp;°C für durchschnittliches Klima-=-Allgemein-=-Saisonale Effizienzklasse Raumheizen","","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++","A++"]
["","Wasserauslass 35°C für durchschnittliches Klima","Allgemein","SCOP","","4.81","4.81","4.81","4.81","4.84","4.84","4.84","4.84","4.84","4.84","4.84","4.84"]
["","","","Saisonale Effizienzklasse Raumheizen","","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++","A+++"]
["Hinweise","","","","","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)","(1) - Bedingung 1: Kühlen: Ta 35°C - LWE 18°C (DT = 5°C); Heizen: Ta TK/FK 7°C/6°C - LWC 35°C (DT = 5°C)"]
["","","","","","(2) - 7 °C/6 °C TK/FK – LWC 35 °C (dT = 5 °C) bei Pumpe auf voller Drehzahl","(2) - 7 °C/6 °C TK/FK – LWC 35 °C (dT = 5 °C) bei Pumpe auf voller Drehzahl","(2) - 7°C/6°CTK/FK– LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl","(2) - 7°C/6°CTK/FK– LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl","(2) - 7 °C/6 °C TK/FK – LWC 35 °C (dT = 5 °C) bei Pumpe auf voller Drehzahl","(2) - 7 °C/6 °C TK/FK – LWC 35 °C (dT = 5 °C) bei Pumpe auf voller Drehzahl","(2) - 7°C/6°CTK/FK– LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl","(2) - 7°C/6°CTK/FK– LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl","(2) - 7 °C/6 °C TK/FK – LWC 35 °C (dT = 5 °C) bei Pumpe auf voller Drehzahl","(2) - 7 °C/6 °C TK/FK – LWC 35 °C (dT = 5 °C) bei Pumpe auf voller Drehzahl","(2) - 7°C/6°CTK/FK– LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl","(2) - 7°C/6°CTK/FK– LWC35°C (dT=5°C) bei Pumpe auf voller Drehzahl"]