{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":9,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSH12E"]
[]
[]
[]
[]
["","","","","","ETSH12P30EG","ETSH12P50EG","ETSH12P30EF","ETSH12P50EF"]
["Gehäuse","Farbe","","","","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)","Verkehrsweiß (RAL 9016) / Verkehrsschwarz (RAL 9017)"]
["","Material","","","","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen","Schlagfestes Polypropylen"]
["Abmessungen","Maßeinheit","","Höhe","mm","1,891","1,910","1,892","1,910"]
["","","","Breite","mm","594","792","594","792"]
["","","","Tiefe","mm","644","817","644","816"]
["Gewicht","Maßeinheit","","","kg","75","98","75","98"]
["Schallleistungspegel","Nom.","","","dB(A)","47.3","47.3","47.3","47.3"]
["Schalldruckpegel","Nom.","","","dB(A)","38.6","38.6","38.6","38.6"]
["Betriebsbereich","Heizen","Wasserseite","Min.","°C","0 (2)","0 (2)","0","0"]
["","","","Max.","°C","0 (2)","0 (2)","0","0"]
["","Kühlung","Umgebung","Min.","°CTK","0 (2)","0 (2)","0","0"]
["","","Wasserseite","Min.","°C","0 (2)","0 (2)","0","0"]
["","","","Max.","°C","0 (2)","0 (2)","0","0"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","230","230","230","230"]
["Hinweise","","","","","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897"]
["","","","","","(2) - Siehe Zeichnungen zu Betriebsgrenzen","(2) - Siehe Zeichnungen zu Betriebsgrenzen","(2) - Siehe Zeichnungen zu Betriebsgrenzen","(2) - Siehe Zeichnungen zu Betriebsgrenzen"]