{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","ETSHB-D"]
[]
[]
[]
[]
["","","","","","ETSHB16P30DA","ETSHB16P50DA"]
["Schalldruckpegel","Nom.","","","dB(A)","32.8","32.8"]
["Betriebsbereich","Kühlung","Umgebung","Min.","°CTK","10","10"]
["","","Wasserseite","Max.","°C","22","22"]
["","","","Min.","°C","5","5"]
["","Heizen","Wasserseite","Max.","°C","70","70"]
["","","","Min.","°C","15","15"]
["Sound power level","Nom.","","","dB(A)","45.6","45.6"]
["Abmessungen","Maßeinheit","","Breite","mm","590","785"]
["","","","Tiefe","mm","615","785"]
["","","","Höhe","mm","1,891","1,896"]
["Gehäuse","Material","","","","Schlagfestes Polypropylen","Schlagfestes Polypropylen"]
["","Farbe","","","","Verkehrsweiß (RAL9016) / Eisengrau (RAL7011)","Verkehrsweiß (RAL9016) / Eisengrau (RAL7011)"]
["PED","Kategorie","","","","Art 4.3","Art 4.3"]
["Gewicht","Maßeinheit","","","kg","75","96"]
["Power supply","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["","Spannung","","","V","230","230"]
["Elektroheizung","Spannungsversorgung","","Frequenz","Hz","50","50"]
["","","","Bezeichnung","","3V / 9W","3V / 9W"]
["","","","Phase","","1~ / 3~","1~ / 3~"]
["Hinweise","","","","","(1) - Wärmeverlust gemäß EN12897","(1) - Wärmeverlust gemäß EN12897"]
["","","","","","(2) - T KW = 10 °C / T WW = 40 °C / T SP = 50 °C","(2) - T KW = 10 °C / T WW = 40 °C / T SP = 50 °C"]
["","","","","","(3) - T KW = 10 °C / T WW = 40 °C / T SP = 60 °C","(3) - T KW = 10 °C / T WW = 40 °C / T SP = 60 °C"]
["","","","","","(4) - T KW = 10 °C / T WW = 40 °C / T SP = 65 °C","(4) - T KW = 10 °C / T WW = 40 °C / T SP = 65 °C"]