{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":7,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAA-B"]
[]
[]
[]
[]
["","","","","","FAA71BUV1B","FAA100BUV1B"]
["Gehäuse","Farbe","","","","Weiß","Weiß"]
["","Material","","","","Kunststoff","Kunststoff"]
["Abmessungen","Maßeinheit","","Höhe","mm","290","340"]
["","","","Breite","mm","1050","1200"]
["","","","Tiefe","mm","269","262"]
["Gewicht","Maßeinheit","","","kg","14","18"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","16.2","23"]
["","","Kühlen","Mittel","m³/min","13.4","21.1"]
["","","","Niedrig","m³/min","12.1","18.7"]
["","","Heizen","Hoch","m³/min","16.9","23"]
["","","","Mittel","m³/min","14.2","20.9"]
["","","","Niedrig","m³/min","12.7","18.7"]
["Schallleistungspegel","Kühlung","","","dBA","61","65"]
["","Heizen","","","dBA","61","65"]
["Schalldruckpegel","Kühlung","","Hoch","dBA","45","49"]
["","Kühlen","","Mittel","dBA","42","45"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dBA","40","41"]
["","Heizen","","Hoch","dBA","45","49"]
["","","","Mittel","dBA","42","45"]
["","","","Niedrig","dBA","40","41"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","9.52"]
["","Gas","","AD","mm","15.9","15.9"]
["","Ableitung","","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Stromversorgung","Phase","","","","1~","1~"]
["","Frequenz","","","Hz","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240"]
["Standardzubehör","Installation plate","","","","1","1"]
["","General safety precautions","","","","1","1"]
["","Wire clamp material","","","","4","4"]
["","Heat insulating tape","","","","1","1"]
["","Installation and operation manual","","","","1","1"]
["","Screw bag","","","","1","1"]
["Hinweise","","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["Standardzubehör","Screw cover","","","","","3"]