{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FAQ-C9"]
[]
[]
[]
[]
["","","","","FAQ71CVEB9","FAQ100CVEB9"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","45","49"]
["","","Nom.","dB(A)","42","45"]
["","","Mittel","dB(A)","42","45"]
["","","Niedrig","dB(A)","40","41"]
["","Kühlung","Medium","dB(A)","42","45"]
["","","Niedrig","dB(A)","40","41"]
["","","Hoch","dB(A)","45","49"]
["","","Nom.","dB(A)","42","45"]
["Kühlleistung","Gesamtleistung","Nom.","kW","0.051","0.061"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","9.52","9.52"]
["","Gas","AD","mm","15.9","15.9"]
["","Ableitung","","","VP13 (I.D. 13/O.D. 18)","VP13 (I.D. 13/O.D. 18)"]
["Sound power level","Kühlung","","dB(A)","61","65"]
["","Heizen","","dB(A)","61","65"]
["Abmessungen","Maßeinheit","Breite","mm","1,050","1,200"]
["","","Tiefe","mm","238","240"]
["","","Höhe","mm","290","340"]
["Gehäuse","Material","","","Kunststoff","Kunststoff"]
["","Farbe","","","Reinweiß","Reinweiß"]
["Gewicht","Maßeinheit","","kg","13","17"]
["Heizleistung","Gesamtleistung","Nom.","kW","0.068","0.061"]
["Power supply","Phase","","","1~","1~"]
["","Frequenz","","Hz","50","50"]
["","Spannung","","V","220-240","220-240"]