{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9) / 4MXM-A"]
[]
[]
[]
[]
["","","","","FBA35A2VEB9 / FBA35A2VEB9 / 4MXM68A2V1B"]
["Kühlleistung","Nom.","","kW","6.8"]
["Raumkühlen","SEER","","","5.26"]
["","Jährlicher Energieverbrauch","","kWh/a","453"]
["","Leistung","Pdesign","kW","6.80"]
["","Energieeffizienzklasse","","","A"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","3.60"]
["","SCOP/A","","","3.81"]
["","Energieeffizienzklasse","","","A"]
["","Jährlicher Energieverbrauch","","kWh/a","1,323"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","1,245"]
["","EER","","","2.73"]
["","COP","","","3.24"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","D"]
["","","Heizen","","C"]
["Heizleistung","Nom.","","kW","8.60"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]