{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9)"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB9","FBA50A2VEB9","FBA60A2VEB9","FBA71A2VEB9","FBA100A2VEB","FBA125A2VEB","FBA140A2VEB"]
["Kühlleistung","Gesamtleistung","","Nom.","kW","","","","","","14.00","15.40"]
["Heizleistung","Gesamtleistung","","Nom.","kW","","","","","","13.5","15.5"]
["Gehäuse","Farbe","","","","Ohne Farbauftrag (galvanisiert)","Ohne Farbauftrag (galvanisiert)","Ohne Farbauftrag (galvanisiert)","Ohne Farbauftrag (galvanisiert)","Ohne Farbauftrag (galvanisiert)","Ohne Farbauftrag (galvanisiert)","Ohne Farbauftrag (galvanisiert)"]
["","Material","","","","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_","Galvanisiertes Stahlblech_"]
["Abmessungen","Maßeinheit","","Höhe","mm","245","245","245","245","245","245","245"]
["","","","Breite","mm","700","700","1000","1000","1400","1400","1400"]
["","","","Tiefe","mm","800","800","800","800","800","800","800"]
["Gewicht","Maßeinheit","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","","Kühlen","Mittel","m³/min","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","","Niedrig","m³/min","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","","Heizen","Hoch","m³/min","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","","","Mittel","m³/min","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","","Niedrig","m³/min","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","Externer statischer Druck","","Nom.","Pa","30","30","30","30","40","50","50"]
["Schallleistungspegel","Kühlung","","","dB(A)","60.0","60.0","56.0","56.0","58.0","62.0","62.0"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","35.0","35.0","30.0","30.0","34.0","37.0","37.0"]
["","Kühlen","","Mittel","dB(A)","32.0","32.0","28.0","","32.0","35.0","35.0"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["","Heizen","","Hoch","dB(A)","37.0","37.0","31.0","31.0","36.0","38.0","38.0"]
["","","","Mittel","dB(A)","34.0","34.0","28.0","","33.0","35.0","35.0"]
["","","","Niedrig","dB(A)","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gas","","AD","mm","9.52","12.70","12.70","15.90","15.90","15.90","15.90"]
["","Ableitung","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Entleerungshöhe","mm","","","","625","625","625","625","625","625","625"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Verkabelte Fernbedienung","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardzubehör","Installation manual","","","","1","1","1","","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","","8","8","8"]
["","Operation manual","","","","1","1","1","","1","1","1"]
["","Clamps","","","","4","4","4","","4","4","4"]
["","Drain hose","","","","1","1","1","","1","1","1"]
["","Insulation for fitting","","","","2","2","2","","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","","1","1","1"]
["","Screws","","","","40","40","40","","40","40","40"]
["","Sealing pads","","","","5","5","5","","5","5","5"]
["Stromversorgung","Phase","","","","1~","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["Spannungsversorgung","Spannung","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Schalldruckpegel","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","","","","28.0"]
["","Heizen","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","","","","28.0"]
["Standardzubehör","Installationsanleitung","","","","","","","1"]
["","Unterlegscheibe für Aufhängung","","","","","","","8"]
["","Bedienungsanleitung","","","","","","","1"]
["","Klemmen","","","","","","","4"]
["","Kondensatschlauch","","","","","","","1"]
["","Isolierung für die Armatur","","","","","","","2"]
["","Metallklemme für Kondensatschlauch","","","","","","","1"]
["","Schrauben","","","","","","","40"]
["","Dichtungsmatten","","","","","","","5"]
["Hinweise","","","","","","","","(1) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt."]
["","","","","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten"]