{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":23,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100BVEB / RZQG100L8Y1B","FCAG125BVEB / RZQG125L8Y1B","FCAG140BVEB / RZQG100L8Y1B","FCAG140BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG125L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG60BVEB / FCAG60BVEB / RZQG125L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG100L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG100L8Y1B","FCAG50BVEB / FCAG50BVEB / FCAG50BVEB / RZQG100L8Y1B","FCAG71BVEB / FCAG71BVEB / RZQG125L8Y1B","FCAG50BVEB / FCAG50BVEB / RZQG71L8Y1B","FCAG100BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG71BVEB / RZQG71L8Y1B","FCAG35BVEB / FCAG35BVEB / FCAG35BVEB / RZQG71L8Y1B","FCAG140BVEB / RZQG140L7Y1B"]
["Energieeffizienzbereich","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Kühlleistung","Nom.","","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["Nominale Effizienz","EER","","","","","","","","","","","","","","","","3.30","3.39","3.30","3.39","3.30","2.50"]
["Raumkühlen","Energieeffizienzklasse","","","","","","","","","","","","","","","","A","A++","A","A++","A"]
["","Leistung","Pdesign","kW","","","","","","","","","","","","","","6.80","6.80","6.80","6.80","6.80","13.40"]
["","SEER","","","","","","","","","","","","","","","","5.10","6.80","5.10","6.72","5.10","6.44"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","","","","467","350","467","355","467","1,249"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","","","","","","","","","","","","","A","A+","A","A+","A"]
["","Leistung","Pdesign","kW","","","","","","","","","","","","","","6.00","6.33","6.00","6.33","6.00","11.56"]
["","SCOP/A","","","","","","","","","","","","","","","","3.80","4.20","3.80","4.20","3.80","4.27"]
["","Jährlicher Energieverbrauch","","kWh/a","","","","","","","","","","","","","","2,211","2,110","2,211","2,110","2,211","3,795"]
["Hinweise","","","","","","","","","","","","","","","","","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Siehe separate Zeichnung für den Betriebsbereich","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","","","","","","","","","","","","","","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Siehe separate Zeichnung für die elektrischen Daten","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","","","","","","","","","","","","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","","","","","","","","","","","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]
["Heizleistung","Nom.","","kW","","","","","","","","","","","","","","","","","7.50","","15.50"]
["Nominale Effizienz","COP","","","","","","","","","","","","","","","","","","","3.97","","3.61"]
["","Jährlicher Energieverbrauch","","kWh","","","","","","","","","","","","","","","","","1,003"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","","","","","","","","","","","","","","","A"]
["","","Heizen","","","","","","","","","","","","","","","","","","A"]