{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":14,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQG-F / RZQG-L7V1/LY1"]
[]
[]
[]
[]
["","","","","FCQG71FVEB / RZQG71L7V1B","FCQG71FVEB / RZQG71L7Y1B9","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG100L7Y1B","FCQG50FVEB / FCQG50FVEB / RZQG100L7V1B","FCQG100FVEB / RZQG100L7V1B","FCQG100FVEB / RZQG100L7Y1B","FCQG50FVEB / FCQG50FVEB / RZQG100L7Y1B","FCQG60FVEB / FCQG60FVEB / RZQG125L7Y1B","FCQG50FVEB / FCQG50FVEB / FCQG50FVEB / RZQG125L7Y1B","FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / FCQG35FVEB / RZQG125L7V1B"]
["Kühlleistung","Nom.","","kW","6.8","6.8","","","9.5","9.5"]
["Raumkühlen","SEER","","","5.81","5.81","4.30","4.30","5.99","5.99","4.30","4.30","4.30","4.30"]
["","Jährlicher Energieverbrauch","","kWh/a","409.639","409.639","773.256","773.256","555.092","555.092","773.256","976.744","976.744","976.744"]
["","Leistung","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Energieeffizienzklasse","","","A+","A+","C","C","A+","A+","C","C","C","C"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","6.33","6.33","10.20","10.20","11.30","11.30","10.20","12.71","12.71","12.71"]
["","SCOP/A","","","4.13","4.13","3.80","3.80","3.93","3.93","3.80","3.40","3.40","3.40"]
["","Energieeffizienzklasse","","","A+","A+","A","A","A","A","A","A","A","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,145.763","2,145.763","3,757","3,757","4,027","4,027","3,757","5,232","5,232","5,232"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","1,005","1,005","","","1,225","1,225"]
["","EER","","","3.39","3.39","","","3.87","3.87"]
["","COP","","","3.97","3.97","","","4.15","4.15"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A","","","A","A"]
["","","Heizen","","A","A","","","A","A"]
["Heizleistung","Nom.","","kW","7.5","7.5","","","10.8","10.8"]
["Hinweise","","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]