{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCQHG71FVEB / RZQG71L8Y1B","FCQHG100FVEB / RZQG71L8Y1B","FCQHG140FVEB / RZQG100L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG100L8Y1B","FCQHG71FVEB / FCQHG71FVEB / RZQG125L8Y1B","FCQHG140FVEB / RZQG125L8Y1B","FCQHG140FVEB / RZQG140L7Y1B"]
["Kühlleistung","Nom.","","kW","6.80","","","","","","13.4"]
["Raumkühlen","SEER","","","6.91","7.00","7.00","5.10","5.10","6.61"]
["","Jährlicher Energieverbrauch","","kWh/a","345","340","475","652","824","636"]
["","Leistung","Pdesign","kW","6.80","6.80","9.50","9.50","12.00","12.00"]
["","Energieeffizienzklasse","","","A++","A++","A++","B","B","A++"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","7.60","7.60","11.30","11.30","12.71","12.66"]
["","SCOP/A","","","4.54","4.54","4.80","3.80","3.80","4.63"]
["","Energieeffizienzklasse","","","A+","A+","A++","A","A","A++"]
["","Jährlicher Energieverbrauch","","kWh/a","2,344","2,344","3,296","4,164","4,683","3,829"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","830"]
["","EER","","","4.09","","","","","","3.35"]
["","COP","","","4.80","","","","","","4.12"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Heizleistung","Nom.","","kW","7.5","","","","","","15.5"]
["Hinweise","","","","(1) - Jährlicher Energieverbrauch gemäß der Energieetikett-Richtlinie 2002/31/EC","","","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - SEER und SCOP gemäß EN 14825","","","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]