{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":116,"n_cols":9,"rows_kept":116,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","","44","45","45"]
["","","","Nom.","dB(A)","","39","40","41"]
["","","","Niedrig","dB(A)","","33","35","37"]
["","Kühlung","","Niedrig","dB(A)","","33","35","37"]
["","","","Hoch","dB(A)","","44","45","45"]
["","","","Nom.","dB(A)","","39","40","41"]
["Standardzubehör","Bedienungsanleitung","","","","","Bedienungsanleitung","Bedienungsanleitung","Bedienungsanleitung"]
["","Installationsanleitung","","","","","Installationsanleitung","Installationsanleitung","Installationsanleitung"]
["","Kondensatschlauch","","","","","Kondensatschlauch","Kondensatschlauch","Kondensatschlauch"]
["","Klemme für Kondensatschlauch","","","","","Klemme für Kondensatschlauch","Klemme für Kondensatschlauch","Klemme für Kondensatschlauch"]
["","Unterlegscheibe für Aufhängung","","","","","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung","Unterlegscheibe für Aufhängung"]
["","Schrauben","","","","","Schrauben","Schrauben","Schrauben"]
["","Isolierung für die Armatur","","","","","2","2","2"]
["","Dichtungsmatten","","","","","4","4","4"]
["","Ablaufdichtungsmatte","","","","","Ablaufdichtungsmatte","Ablaufdichtungsmatte","Ablaufdichtungsmatte"]
["","Klemmen","","","","","Klemmen","Klemmen","Klemmen"]
["Control systems","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","","9.52","9.52","9.52"]
["","Gas","","AD","mm","","15.9","15.9","15.9"]
["","Ableitung","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Geräteblende 4","Abmessungen","","Tiefe","mm","","50","50","50"]
["","","","Breite","mm","","950","950","950"]
["","","","Höhe","mm","","950","950","950"]
["","Modell","","","","","BYCQ140D7W1 – Weiß mit grauen Lamellen","BYCQ140D7W1 – Weiß mit grauen Lamellen","BYCQ140D7W1 – Weiß mit grauen Lamellen"]
["","Farbe","","","","","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)"]
["","Gewicht","","","kg","","5.4","5.4","5.4"]
["Sound power level","Kühlung","","","dB(A)","","61","61","61"]
["","Heizen","","","dB(A)","","61","61","61"]
["Abmessungen","Maßeinheit","","Breite","mm","","840","840","840"]
["","","","Tiefe","mm","","840","840","840"]
["","","","Höhe","mm","","288","288","288"]
["Casing","Material","","","","","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech."]
["Gewicht","Maßeinheit","","","kg","","26","26","26"]
["Geräteblende","Gewicht","","","kg","","10.3","10.3","10.3"]
["","Modell","","","","","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter"]
["","Abmessungen","","Höhe","mm","","130","130","130"]
["","","","Tiefe","mm","","950","950","950"]
["","","","Breite","mm","","950","950","950"]
["","Farbe","","","","","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)","Reinweiß (RAL 9010)"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Frequenz","","","Hz","","50","50","50"]
["","Bezeichnung","","","","","VE","VE","VE"]
["","Spannung","","","V","","220-240","220-240","220-240"]
["Hinweise","","","","","","(1) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(1) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(1) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt."]
["","","","","","","(2) - Das BYCQ140D7W1W verfügt über eine weiße Isolation. Beachten Sie, dass Schmutz auf weißem Isolationsmaterial stärker zu sehen ist und daher eine Installation der Zierblende BYCQ140D7W1W in staubreichen Umgebungen nicht empfehlenswert ist.","(2) - Das BYCQ140D7W1W verfügt über eine weiße Isolation. Beachten Sie, dass Schmutz auf weißem Isolationsmaterial stärker zu sehen ist und daher eine Installation der Zierblende BYCQ140D7W1W in staubreichen Umgebungen nicht empfehlenswert ist.","(2) - Das BYCQ140D7W1W verfügt über eine weiße Isolation. Beachten Sie, dass Schmutz auf weißem Isolationsmaterial stärker zu sehen ist und daher eine Installation der Zierblende BYCQ140D7W1W in staubreichen Umgebungen nicht empfehlenswert ist."]
["","","","","","","(3) - BYCQ140D7W1: Reinweiße Standardblende mit grauen Lamellen; BYCQ140D7W1W: Reinweiße Standardblende mit weißen Lamellen; BYCQ140D7GW1: Reinweiße Blende mit Funktion zur automatischen Reinigung","(3) - BYCQ140D7W1: Reinweiße Standardblende mit grauen Lamellen; BYCQ140D7W1W: Reinweiße Standardblende mit weißen Lamellen; BYCQ140D7GW1: Reinweiße Blende mit Funktion zur automatischen Reinigung","(3) - BYCQ140D7W1: Reinweiße Standardblende mit grauen Lamellen; BYCQ140D7W1W: Reinweiße Standardblende mit weißen Lamellen; BYCQ140D7GW1: Reinweiße Blende mit Funktion zur automatischen Reinigung"]
["Gehäuse","Material","","","","Galvanisiertes Stahlblech_"]
["Abmessungen","Maßeinheit","","Höhe","mm","288"]
["","","","Breite","mm","840"]
["","","","Tiefe","mm","840"]
["Gewicht","Maßeinheit","","","kg","25"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Niedrig","m³/min","12.2"]
["","","Heizen","Hoch","m³/min","21.2"]
["","","","Nom.","m³/min","16.7"]
["","","","Niedrig","m³/min","12.2"]
["Schallleistungspegel","Kühlung","","","dB(A)","53"]
["","Heizen","","","dB(A)","53"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","36"]
["","","","Nom.","dB(A)","33"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","29"]
["","Heizen","","Hoch","dB(A)","36"]
["","","","Nom.","dB(A)","33"]
["","","","Niedrig","dB(A)","29"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52"]
["","Gas","","AD","mm","15.9"]
["","Ableitung","","","","VP25 (I.D. 25/O.D. 32)"]
["Geräteblende","Modell","","","","BYCQ140D7GFW1 – selbstreinigende Zierblende mit feinmaschigem Filter"]
["","Farbe","","","","Reinweiß (RAL 9010)"]
["","Abmessungen","","Höhe","mm","130"]
["","","","Breite","mm","950"]
["","","","Tiefe","mm","950"]
["","Gewicht","","","kg","10.3"]
["Geräteblende 2","Modell","","","","BYCQ140D7GW1 – Selbstreinigende Zierblende"]
["","Farbe","","","","Reinweiß (RAL 9010)"]
["","Abmessungen","","Höhe","mm","130"]
["","","","Breite","mm","950"]
["","","","Tiefe","mm","950"]
["","Gewicht","","","kg","10.3"]
["Geräteblende 3","Modell","","","","BYCQ140D7W1W – Vollweiß"]
["","Farbe","","","","Reinweiß (RAL 9010)"]
["","Abmessungen","","Höhe","mm","50"]
["","","","Breite","mm","950"]
["","","","Tiefe","mm","950"]
["","Gewicht","","","kg","5.4"]
["Geräteblende 4","Modell","","","","BYCQ140D7W1 – Weiß mit grauen Lamellen"]
["","Farbe","","","","Reinweiß (RAL 9010)"]
["","Abmessungen","","Höhe","mm","950"]
["","","","Breite","mm","950"]
["","","","Tiefe","mm","50"]
["","Gewicht","","","kg","5.4"]
["Control systems","Infrared remote control","","","","BRC7FA532F"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC1D52, BRC1E52A/B"]
["Standardzubehör","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Stromversorgung","Bezeichnung","","","","VE"]
["","Phase","","","","1~"]
["","Stromversorgung-=-Frequenz","","Frequenz","","50"]
["Spannungsversorgung","Spannungsversorgung-=-Spannung","","Spannung","","220-240"]