{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":66,"n_cols":8,"rows_kept":66,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Kühlleistung","Gesamtleistung","","Nom.","kW","12.10","19.00","22.00"]
["Heizleistung","Gesamtleistung","","Nom.","kW","13.50","22.4","24.0"]
["Gehäuse","Farbe","","","","Unbeschichtet","Unbeschichtet","Unbeschichtet"]
["","Material","","","","Galvanisiertes Stahlblech","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech."]
["Abmessungen","Maßeinheit","","Höhe","mm","300","470","470"]
["","","","Breite","mm","1,400","1,490","1,490"]
["","","","Tiefe","mm","700","1,100","1,100"]
["Gewicht","Maßeinheit","","","kg","45","104","115"]
["Erforderliche Zwischendeckenhöhe >","mm","","","","350"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","39.0","64.0","69.0"]
["","","","Mittel","m³/min","","50","56"]
["","","","Niedrig","m³/min","28.0","36.0","43.0"]
["","","Heizen","Hoch","m³/min","39.0","64.0","69.0"]
["","","","Mittel","m³/min","","50.0","56.0"]
["","","","Niedrig","m³/min","28.0","36.0","43.0"]
["","Externer statischer Druck","","Hoch","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Kühlung","","","dB(A)","66","69.0","71.0"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","40","43.0","44.0"]
["","","","Mittel","dB(A)","","39.0","40.0"]
["","","","Niedrig","dB(A)","33","36.0","37.0"]
["","Heizen","","Hoch","dB(A)","40","43.0","44.0"]
["","","","Mittel","dB(A)","","39.0","40.0"]
["","","","Niedrig","dB(A)","33","36.0","37.0"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","9.52","9.52","9.52"]
["","Gas","","AD","mm","15.90","19.1","22.2"]
["","Ableitung","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Entleerungshöhe","mm","","","","625"]
["Geräteblende","Modell","","","","BYBS125DJW1"]
["","Farbe","","","","Weiß (10Y9/0.5)"]
["","Abmessungen","","Höhe","mm","55"]
["","","","Breite","mm","1,500"]
["","","","Tiefe","mm","500"]
["","Gewicht","","","kg","6.5"]
["Regelungssysteme","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Wired remote control","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardzubehör","Schrauben","","","","16","2","2"]
["","Unterlegscheibe","","","","8","8","8"]
["","Schlauchband","","","","1"]
["","Kondensatschlauch","","","","1"]
["","Allgemeine Schutzmaßnahmen","","","","1","1","1"]
["","Installations- und Bedienungsanleitung","","","","1","1","1"]
["","Kabel für gemeinsame Stromversorgung","","","","2"]
["","Dichtmaterial (Kondensatschlauch)","","","","1"]
["","Dichtungsmaterial","","","","2"]
["","Wärmeisolierrohr (Flüssigkeit)","","","","1"]
["","Wärmeisolierrohr (Gas)","","","","1"]
["Power supply","Bezeichnung","","","","","VE","VE"]
["","Phase","","","","1~","1~","1~"]
["","Frequenz","","","Hz","50/60","50/60","50/60"]
["","Spannung","","","V","220-240/220","220-240/220","220-240/220"]
["Hinweise","","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["Standardzubehör","Bedienungsanleitung","","","","","1","1"]
["","Installationsanleitung","","","","","1","1"]
["","Gasanschlussleitung","","","","","1","1"]
["","Material Kabelklemme","","","","","1","1"]
["","Federscheibe","","","","","2","2"]
["","Schraube + Unterlegscheibe","","","","","45","45"]
["","Sechskantschraube mit Unterlegscheibe","","","","","49","49"]
["","Sechskantschraube","","","","","2","2"]