{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L8V1B"]
["Kühlleistung","Nom.","","kW","12.0"]
["Raumkühlen","SEER","","","5.20"]
["","Jährlicher Energieverbrauch","","kWh/a","807.692"]
["","Leistung","Pdesign","kW","12.00"]
["","Energieeffizienzklasse","","","A"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","7.60"]
["","SCOP/A","","","3.90"]
["","Energieeffizienzklasse","","","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,728.205"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","1,870"]
["","EER","","","3.21"]
["","COP","","","3.51"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","B"]
["Heizleistung","Nom.","","kW","13.5"]
["Hinweise","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]