{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":7,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-C / RZQSG-LV1/LY1"]
[]
[]
[]
[]
["","","","","FDQ125C7VEB / RZQSG125L7V1B","FDQ125C7VEB / RZQSG125L7Y1B9","FDQ125C7VEB / RZQSG125L7Y1B"]
["Kühlleistung","Nom.","","kW","12.0","12.0","12.0 (3)"]
["Raumkühlen","SEER","","","4.35","4.35","4.35 (6)"]
["","Jährlicher Energieverbrauch","","kWh/a","965.517","965.517"]
["","Leistung","Pdesign","kW","12.00","12.00"]
["","Energieeffizienzklasse","","","C","C"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","7.60","7.60"]
["","SCOP/A","","","3.81","3.81","3.81 (6)"]
["","Energieeffizienzklasse","","","A","A"]
["","Jährlicher Energieverbrauch","","kWh/a","2,791","2,791"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","1,870","1,600","1,870"]
["","EER","","","3.21","3.21","3.21"]
["","COP","","","3.51","3.51","3.51"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A","A"]
["","","Heizen","","B","B","B"]
["Heizleistung","Nom.","","kW","13.5","13.5","13.5 (4)"]
["Hinweise","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - Jährlicher Energieverbrauch: auf der Grundlage von etwa 500 Betriebsstunden pro Jahr bei Volllast (Nennbedingungen)"]
["","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","(2) - Energieetikett: Skala von A (am effizientesten) bis G (am wenigsten effizient)"]
["","","","","","","(3) - Kühlen: Innentemperatur: 27°C TK, 19°C FK, Außentemp. 35°C TK, äquivalente Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","","","(4) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m"]
["","","","","","","(5) - Jährlicher Energieverbrauch gemäß der Energieetikett-Richtlinie 2002/31/EC"]
["","","","","","","(6) - SEER und SCOP gemäß EN 14825"]
["","","","","","","(7) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]