{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXS50L2V1B","FDXM60F3V1B / RXS60L2V1B"]
["Kühlleistung","Nom.","","kW","5.00","6.00"]
["Raumkühlen","SEER","","","5.72","5.51"]
["","Jährlicher Energieverbrauch","","kWh/a","306","381"]
["","Leistung","Pdesign","kW","5.00","6.00"]
["","Energieeffizienzklasse","","","A+","A"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","4.00","4.60"]
["","SCOP/A","","","3.93","3.80"]
["","Energieeffizienzklasse","","","A","A"]
["","Jährlicher Energieverbrauch","","kWh/a","1,425","1,693"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35"]
["","Gas","AD","mm","12.70","12.70"]
["","Ableitung","OD","mm","VP20 (Außendurchmesser 26, Innendurchmesser 20)","VP20 (Außendurchmesser 26, Innendurchmesser 20)"]
["Nominale Effizienz","EER","","","3.03","2.91"]
["","Jährlicher Energieverbrauch","","kWh","825","1,030"]
["","COP","","","3.10","3.21"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","B","C"]
["","","Heizen","","D","C"]
["Heizleistung","Nom.","","kW","5.80","7.00"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]