{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":6,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXM-A"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B9 / RXM50A5V1B","FDXM60F3V1B9 / RXM60A5V1B"]
["Kühlleistung","Min.","","kW","1.70","1.7"]
["","Nom.","","kW","5.00","6"]
["","Max.","","kW","5.30","6.5"]
["Heizleistung","Min.","","kW","1.70","1.7"]
["","Nom.","","kW","5.80","7"]
["","Max.","","kW","6.00","7.1"]
["Nominale Effizienz","EER","","","3.06","2.93"]
["","COP","","","3.10","3.21"]
["","Jährlicher Energieverbrauch","","kWh","817","1024"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","B","C"]
["","","Heizen","","D","C"]
["Raumkühlen","Energieeffizienzklasse","","","A+","A"]
["","Leistung","Pdesign","kW","5.00","6"]
["","SEER","","","5.77","5.56"]
["","Jährlicher Energieverbrauch","","kWh/a","303","378"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A","A"]
["","Leistung","Pdesign","kW","4.00","4.6"]
["","SCOP/A","","","3.93","3.8"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung&nbsp;Pdh bei&nbsp;-10°-=-kW","","kW","3.54","3.94"]
["","Jährlicher Energieverbrauch","","kWh/a","1424","1693"]
["Hinweise","","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten"]