{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9 / RXS-L3"]
[]
[]
[]
[]
["","","","","FDXM25F3V1B9 / RXS25L3V1B","FDXM35F3V1B9 / RXS35L3V1B"]
["Kühlleistung","Min.","","kW","1.30","1.40"]
["","Max.","","kW","3.00","3.80"]
["","Nom.","","kW","2.40","3.40"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35"]
["","Gas","AD","mm","9.50","9.50"]
["","Ableitung","OD","mm","VP20 (Außendurchmesser 26, Innendurchmesser 20)","VP20 (Außendurchmesser 26, Innendurchmesser 20)"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","321","574"]
["","EER","","","3.74","2.96"]
["","COP","","","4.00","3.48"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","B"]
["","","Heizen","","A","A"]
["Heizleistung","Nom.","","kW","3.20","4.00"]
["","Min.","","kW","1.30","1.40"]
["","Max.","","kW","4.50","5.00"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]