{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Schalldruckpegel","Heizen","Hoch","dBA","38"]
["","","Mittel","dBA","36"]
["","","Niedrig","dBA","30"]
["","Kühlung","Medium","dBA","36"]
["","","Niedrig","dBA","30"]
["","","Hoch","dBA","38"]
["Standardzubehör","Installationsanleitung","","","1"]
["","Bedienungsanleitung","","","1"]
["","Isolierung für die Armatur","","","1"]
["","Dichtungsmatte","","","1"]
["","Klemmblech","","","1"]
["","Kondensatschlauch","","","1"]
["","Unterlegscheibe für Aufhängung","","","8"]
["","Dichtungsmaterial","","","2"]
["","Klemmen","","","6"]
["","Unterlegscheibe für Befestigungsplatte","","","4"]
["","Schrauben für Kanalflansche","","","1"]
["","Luftfilter","","","1"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35"]
["","Gas","AD","mm","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)"]
["Leistungsaufnahme","Kühlung","Nom.","kW","0.060"]
["","Heizen","Nom.","kW","0.060"]
["Sound power level","Kühlung","","dBA","55"]
["","Heizen","","dBA","55"]
["Abmessungen","Maßeinheit","Breite","mm","1,150"]
["","","Tiefe","mm","620"]
["","","Höhe","mm","200"]
["Gewicht","Maßeinheit","","kg","30.0"]
["Ventilator","Externer statischer Druck","Nom.","Pa","40"]
["Power supply","Phase","","","1~"]
["","Frequenz","","Hz","50/60"]
["","Bezeichnung","","","VE"]
["","Spannung","","V","220-240"]
["Hinweise","","","","(1) - Bei Anschluss an einem Multi-Außengerät lesen Sie bitte die technischen Gerätedaten des anzuschließenden Multi-Außengeräts."]