{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":8,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FFA25A2VEB / RXM25M3V1B9","FFA35A2VEB / RXM35M3V1B9","FFA50A2VEB / RXM50M3V1B9","FFA60A2VEB / RXM60M3V1B9"]
["Kühlleistung","Nom.","","kW","2.50","3.40"]
["Raumkühlen","SEER","","","6.17","6.38"]
["","Jährlicher Energieverbrauch","","kWh/a","142","186"]
["","Leistung","Pdesign","kW","2.50","3.40"]
["","Energieeffizienzklasse","","","A++","A++"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","2.31","3.10"]
["","SCOP/A","","","4.24","4.10"]
["","Energieeffizienzklasse","","","A+","A+"]
["","Jährlicher Energieverbrauch","","kWh/a","762","1,058"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","273","446"]
["","EER","","","4.57","3.81"]
["","COP","","","3.90","3.50"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","B"]
["Heizleistung","Nom.","","kW","3.20","4.20"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(3) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(3) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["Outdoor unit","","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Kühlleistung","Nom.","","kW","","","5.00","5.70"]
["Heizleistung","Nom.","","kW","","","5.80","7.00"]
["Nominale Effizienz","EER","","","","","3.24","3.05"]
["","COP","","","","","3.49","3.41"]
["","Jährlicher Energieverbrauch","","kWh","","","771","934"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","","A","B"]
["","","Heizen","","","","B","B"]
["Raumkühlen","Energieeffizienzklasse","","","","","A+","A+"]
["","Leistung","Pdesign","kW","","","5.00","5.70"]
["","SEER","","","","","5.98","5.76"]
["","Jährlicher Energieverbrauch","","kWh/a","","","292","347"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","","A","A+"]
["","Leistung","Pdesign","kW","","","3.84","3.96"]
["","SCOP/A","","","","","3.90","4.04"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","","3.51","3.66"]
["","Jährlicher Energieverbrauch","","kWh/a","","","1377","1372"]