{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":19,"n_cols":6,"rows_kept":19,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RZASG-MY1"]
[]
[]
[]
[]
["","","","","FFA35A2VEB / FFA35A2VEB / FFA35A2VEB / RZASG100M7Y1B","FFA50A2VEB / FFA50A2VEB / RZASG100M7Y1B"]
["Outdoor unit","","","","RZASG100M7Y1B","RZASG100M7Y1B"]
["Kühlleistung","Nom.","","kW","9.50","9.50"]
["Heizleistung","Nom.","","kW","10.8","10.8"]
["Raumkühlen","Energieeffizienzklasse","","","A++","A"]
["","Leistung","Pdesign","kW","9.50","9.50"]
["","SEER","","","6.24","5.49"]
["","Jährlicher Energieverbrauch","","kWh/a","533","606"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A","A"]
["","Leistung","Pdesign","kW","6.00","6.00"]
["","SCOP/A","","","3.82","3.90"]
["","Jährlicher Energieverbrauch","","kWh/a","2199","2154"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]