{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":6,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A9 / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB9 / RXM50N2V1B","FFA60A2VEB9 / RXM60N2V1B"]
["Kühlleistung","Nom.","","kW","5.00"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","772"]
["","EER","","","3.24"]
["","COP","","","3.49"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Heizleistung","Nom.","","kW","5.80"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Siehe separate Zeichnung für die elektrischen Daten","(4) - Siehe separate Zeichnung für die elektrischen Daten"]
["Outdoor unit","","","","","RXM60N2V1B"]
["Kühlleistung","Nom.","","kW","","5.70"]
["Heizleistung","Nom.","","kW","","7.00"]
["Nominale Effizienz","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Jährlicher Energieverbrauch","","kWh","","934"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","B"]
["","","Heizen","","","B"]
["Raumkühlen","Energieeffizienzklasse","","","","A+"]
["","Leistung","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Jährlicher Energieverbrauch","","kWh/a","","347"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","A+"]
["","Leistung","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","3.66"]
["","Jährlicher Energieverbrauch","","kWh/a","","1372"]
["Energieeffizienzbereich","","","","","A+++ ~ D"]