{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Kühlleistung","Nom.","","kW","3.40"]
["Raumkühlen","SEER","","","6.24"]
["","Jährlicher Energieverbrauch","","kWh/a","191"]
["","Leistung","Pdesign","kW","3.40"]
["","Energieeffizienzklasse","","","A++"]
["Raumheizen (Durchschnittliches Klima)","Leistung","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Energieeffizienzklasse","","","A+"]
["","Jährlicher Energieverbrauch","","kWh/a","979"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Heizleistung","Nom.","","kW","4.00"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten"]
["","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(3) - Nennkühlleistungen basieren auf: Innentemp.: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["Außengerät","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Kühlleistung","Nom.","","kW","","5.00","5.70"]
["Heizleistung","Nom.","","kW","","6.00","7.20"]
["Nominale Effizienz","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Jährlicher Energieverbrauch","","kWh","","780","867"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","","B","A"]
["","","Heizen","","","C","C"]
["Raumkühlen","Energieeffizienzklasse","","","","A+","A+"]
["","Leistung","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Jährlicher Energieverbrauch","","kWh/a","","295","328"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","A","A"]
["","Leistung","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","","3.85","4.08"]
["","Jährlicher Energieverbrauch","","kWh/a","","1578","1704"]