{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":15,"n_cols":6,"rows_kept":15,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RXS-K"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / RXS35K2V1B","FHQ50CAVEB / RXS50K2V1B"]
["Kühlleistung","Nom.","","kW","3.4","5.0"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","475","785"]
["","EER","","","3.58","3.18"]
["","COP","","","3.96","3.35"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","B"]
["","","Heizen","","A","C"]
["Heizleistung","Nom.","","kW","4.0","6.0"]
["Hinweise","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast","(2) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]