{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":5,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9 / RXS-L"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9 / RXS35L2V1B"]
["Kühlleistung","Min.","","kW","1.2"]
["","Max.","","kW","3.8"]
["","Nom.","","kW","3.5"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35"]
["","Gas","AD","mm","9.5"]
["","Ableitung","OD","mm","18.0"]
["Nominale Effizienz","Jährlicher Energieverbrauch","","kWh","565"]
["","EER","","","3.10"]
["","COP","","","3.57"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","B"]
["","","Heizen","","B"]
["Heizleistung","Nom.","","kW","4.0"]
["","Min.","","kW","1.4"]
["","Max.","","kW","5.0"]
["Hinweise","","","","(1) - EER/COP gemäß Eurovent 2012, nur zur Verwendung außerhalb der EU"]
["","","","","(2) - 220 V"]
["","","","","(3) - 230 V"]
["","","","","(4) - 240 V"]
["","","","","(5) - Kühlen: Innentemperatur: 27°C TK, 19,0°C FK; Außentemp. 35°C TK, 24°C FK; äquivalente Leitungslänge: 5 m"]
["","","","","(6) - Heizen: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m"]
["","","","","(7) - Nominale Effizienz: Kühlen bei 35 °C/27 °C Nennlast, Heizen bei 7 °C/20 °C Nennlast"]