{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-R9"]
[]
[]
[]
[]
["","","","","FNA25A2VEB9 / RXM25R5V1B9","FNA35A2VEB9 / RXM35R5V1B9"]
["Kühlleistung","Nom.","","kW","2.60","3.40"]
["Heizleistung","Nom.","","kW","3.20","4.00"]
["Nominale Effizienz","EER","","","3.80","3.09"]
["","COP","","","4.00","3.48"]
["","Jährlicher Energieverbrauch","","kWh","342","550"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","B"]
["","","Heizen","","A","B"]
["Raumkühlen","Energieeffizienzklasse","","","","A+"]
["","Leistung","Pdesign","kW","","3.40"]
["","SEER","","","","5.70"]
["","Jährlicher Energieverbrauch","","kWh/a","","209"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","","A+"]
["","Leistung","Pdesign","kW","","2.90"]
["","SCOP/A","","","","4.05"]
["","Jährlicher Energieverbrauch","","kWh/a","","1,002"]
["Hinweise","","","","(1) - Siehe separate Zeichnung für die elektrischen Daten","(1) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m."]
["","","","","(2) - Siehe separate Zeichnung für den Betriebsbereich","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m."]
["","","","","(3) - Nennkühlleistungen basieren auf: Innentemperatur: 27 °C TK, 19 °C FK; Außentemperatur: 35 °C TK; äquivalente Länge Kältemittelleitung: 5 m; Niveauunterschied: 0 m.","(3) - Siehe separate Zeichnung für den Betriebsbereich"]
["","","","","(4) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5 m; Niveauunterschied: 0 m.","(4) - Siehe separate Zeichnung für die elektrischen Daten"]