{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":9,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9"]
[]
[]
[]
[]
["","","","","","FNA25A2VEB9","FNA35A2VEB9","FNA50A2VEB9","FNA60A2VEB9"]
["Schalldruckpegel","Heizen","","Hoch","dB(A)","33.0","33.0","36.0","36.0"]
["","","","Nom.","dB(A)","31.0","31.0","33.0","33.0"]
["","","","Niedrig","dB(A)","28.0","28.0","30.0","30.0"]
["","Kühlung","","Medium","dB(A)","31.0","31.0","33.0","33.0"]
["","","","Niedrig","dB(A)","28.0","28.0","30.0","30.0"]
["","","","Hoch","dB(A)","33.0","33.0","36.0","36.0"]
["Regelungssysteme","Verkabelte Fernbedienung","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["","Infrared remote control","","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.52","9.52","12.7","12.7"]
["","Ableitung","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Sound power level","Kühlung","","","dB(A)","53.0","53.0","56.0","56.0"]
["Abmessungen","Maßeinheit","","Breite","mm","790","790","1,190","1,190"]
["","","","Tiefe","mm","200","200","200","200"]
["","","","Höhe","mm","620, 720 (1)","620, 720 (1)","620, 720 (1)","620, 720 (1)"]
["Gehäuse","Material","","","","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech.","Galvanisiertes Stahlblech."]
["","Farbe","","","","Unbeschichtet","Unbeschichtet","Unbeschichtet","Unbeschichtet"]
["Gewicht","Maßeinheit","","","kg","23.0","23.0","30.0","30.0"]
["Ventilator","Externer statischer Druck","","Hoch","Pa","48","48","49","49"]
["","","","Nom.","Pa","30","30","40","40"]
["","Luftstromvolumen","Heizen","Hoch","m³/min","8.7","8.7","16.0","16.0"]
["","","","Niedrig","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8.0","8.0","14.8","14.8"]
["","","Kühlung","Niedrig","m³/min","7.3","7.3","13.5","13.5"]
["","","","Nom.","m³/min","8.0","8.0","14.8","14.8"]
["","","","Hoch","m³/min","8.7","8.7","16.0","16.0"]
["Power supply","Phase","","","","1~","1~","1~","1~"]
["","Bezeichnung","","","","VE","VE","VE","VE"]
["","Frequenz","","","Hz","50/60","50/60","50/60","50/60"]
["","Spannung","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Hinweise","","","","","(1) - Einschließlich Installationsfüße","(1) - Einschließlich Installationsfüße","(1) - Einschließlich Installationsfüße","(1) - Einschließlich Installationsfüße"]
["","","","","","(2) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(2) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(2) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt.","(2) - Der Schallleistungspegel ist ein absoluter Wert und gibt die \"Leistung\" an, die eine Schallquelle erzeugt."]