{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":6,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-CS / RXA-A9"]
[]
[]
[]
[]
["","","","","FTXA20C2V1BS / RXA20A5V1B9 (Archived)","FTXA25C2V1BS / RXA25A5V1B9 (Archived)"]
["Kühlleistung","Min.","","kW","1.30","1.30"]
["","Nom.","","kW","2.00","2.50"]
["","Max.","","kW","2.60","3.20"]
["Heizleistung","Min.","","kW","1.30","1.30"]
["","Nom.","","kW","2.50","2.80"]
["","Max.","","kW","3.50","4.70"]
["Nominale Effizienz","EER","","","4.70","4.46"]
["","COP","","","5.00","5.00"]
["","Jährlicher Energieverbrauch","","kWh","213","280"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A","A"]
["","","Heizen","","A","A"]
["Raumkühlen","Energieeffizienzklasse","","","A+++","A+++"]
["","Leistung","Pdesign","kW","2.00","2.50"]
["","SEER","","","8.75","8.74"]
["","Jährlicher Energieverbrauch","","kWh/a","80","100"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A+++","A+++"]
["","Leistung","Pdesign","kW","2.40","2.45"]
["","SCOP/A","","","5.15","5.15"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","2.04","2.09"]
["","Jährlicher Energieverbrauch","","kWh/a","652","666"]
["Energieeffizienzbereich","","","","A+++ ~ D","A+++ ~ D"]