{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":10,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-DL"]
[]
[]
[]
[]
["","","","","","FTXA20D2V1BL","FTXA25D2V1BL","FTXA35D2V1BL","FTXA42D2V1BL","FTXA50D2V1BL"]
["Leistungsaufnahme","Kühlung","","Nom.","kW","0.020","0.022","0.023","0.028","0.030"]
["","Heizen","","Nom.","kW","0.020","0.020","0.220","0.036","0.039"]
["Gehäuse","Farbe","","","","Casing: Black, Panel: Dark brown leather","Casing: Black, Panel: Dark brown leather","Casing: Black, Panel: Dark brown leather","Casing: Black, Panel: Dark brown leather","Casing: Black, Panel: Dark brown leather"]
["Abmessungen","Maßeinheit","","Höhe","mm","295","295","295","295","295"]
["","","","Breite","mm","798","798","798","798","798"]
["","","","Tiefe","mm","189","189","189","189","189"]
["Gewicht","Maßeinheit","","","kg","11.5","11.5","11.5","11.5","11.5"]
["Ventilator","Luftstromvolumen","Kühlung","Hoch","m³/min","11.0","11.5","11.9","13.1","13.5"]
["","","Kühlen","Mittel","m³/min","8.2","8.6","8.6","9.8","10.4"]
["","","","Niedrig","m³/min","6.1","6.1","6.1","7.2","7.6"]
["","","","Flüsterbetrieb","m³/min","4.6","4.6","4.6","4.6","5.2"]
["","","Heizen","Hoch","m³/min","10.9","11.1","11.5","14.6","15.1"]
["","","","Mittel","m³/min","8.7","9.0","9.0","10.5","11.1"]
["","","","Niedrig","m³/min","6.4","6.4","6.4","7.7","8.2"]
["","","","Flüsterbetrieb","m³/min","4.5","4.5","4.5","5.2","5.7"]
["Schallleistungspegel","Kühlung","","","dB(A)","57","57","60","60","60"]
["Schalldruckpegel","Kühlung","","Hoch","dB(A)","39","40","41","45","46"]
["","Kühlen","","Schalldruckpegel-=-Kühlen-=-Mittel-=-dB(A)","dB(A)","32","33","33","37","39"]
["","","","Schalldruckpegel-=-Kühlung-=-Niedrig-=-dB(A)","dB(A)","25","25","25","29","31"]
["","","","Flüsterbetrieb","dB(A)","19","19","19","21","24"]
["","Heizen","","Hoch","dB(A)","39","40","41","45","46"]
["","","","Schalldruckpegel-=-Heizen-=-Mittel-=-dB(A)","dB(A)","32","33","33","37","42"]
["","","","Niedrig","dB(A)","25","25","25","29","33"]
["","","","Flüsterbetrieb","dB(A)","19","19","19","21","24"]
["Kältemittel","GWP","","","","675.0","675.0","675.0","675.0","675.0"]
["Rohrleitungsanschlüsse","Flüssigkeit","","AD","mm","6.35","6.35","6.35","6.35","6.35"]
["","Gas","","AD","mm","9.50","9.50","9.50","9.50","12.7"]
["","Ableitung","","","","18","18","18","18","18"]
["Regelungssysteme","Infrarot-Fernbedienung","","","","ARC466A94","ARC466A94","ARC466A94","ARC466A94","ARC466A94"]
["","Verkabelte Fernbedienung","","","","BRC073A1","BRC073A1","BRC073A1","BRC073A1","BRC073A1"]
["Standardzubehör","Installationsanleitung","","","","1","1","1","1","1"]
["","Schraubenabdeckung","","","","2","2","2","2","2"]
["","Trockenbatterien, Typ AAA","","","","2","2","2","2","2"]
["","Allgemeine Schutzmaßnahmen","","","","1","1","1","1","1"]
["","Bedienungsanleitung","","","","1","1","1","1","1"]
["","Luftfilter","","","","2","2","2","2","2"]
["","Infrarot-Fernbedienung","","","","1","1","1","1","1"]
["","Montageplatte für Fernbedienung","","","","1","1","1","1","1"]
["","Schraubensack","","","","1","1","1","1","1"]
["Energieeffizienzbereich","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Stromversorgung","Bezeichnung","","","","V1","V1","V1","V1","V1"]
["","Phase","","","","1~","1~","1~","1~","1~"]
["","Frequenz","","","Hz","50","50","50","50","50"]
["Spannungsversorgung","Spannung","","","V","220-240","220-240","220-240","220-240","220-240"]