{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-DP / RXA-B9"]
[]
[]
[]
[]
["","","","","FTXA42D2V1BP / RXA42B5V1B9"]
["Kühlleistung","Min.","","kW","1.70"]
["","Nom.","","kW","4.20"]
["","Max.","","kW","5.00"]
["Heizleistung","Min.","","kW","1.70"]
["","Nom.","","kW","5.40"]
["","Max.","","kW","6.00"]
["Nominale Effizienz","EER","","","3.99"]
["","COP","","","4.12"]
["","Jährlicher Energieverbrauch","","kWh","526"]
["","Richtlinie zur Energiekennzeichnung","Kühlen","","A"]
["","","Heizen","","A"]
["Raumkühlen","Energieeffizienzklasse","","","A++"]
["","Leistung","Pdesign","kW","4.20"]
["","SEER","","","7.50"]
["","Jährlicher Energieverbrauch","","kWh/a","196"]
["Raumheizen (Durchschnittliches Klima)","Energieeffizienzklasse","","","A++"]
["","Leistung","Pdesign","kW","3.80"]
["","SCOP/A","","","4.60"]
["","Raumheizen (Durchschnittliches Klima)-=-Heizleistung Pdh bei -10°-=-kW","","kW","3.04"]
["","Jährlicher Energieverbrauch","","kWh/a","1156"]
["Energieeffizienzbereich","","","","A+++ ~ D"]
["Hinweise","","","","(1) - Nennkühlleistungen basieren auf: Innentemp.: 27°CTK, 19°CFK; Außentemperatur: 35°CTK; äquivalente Länge Kältemittelleitung: 5m; Niveauunterschied: 0m."]
["","","","","(2) - Nennheizleistungen basieren auf: Innentemperatur: 20°C TK; Außentemperatur: 7°C TK, 6°C FK; äquivalente Kältemittel-Leitungslänge: 5m; Niveauunterschied: 0 m."]
["","","","","(3) - Siehe separate Zeichnung für den Betriebsbereich"]