{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":47,"n_cols":10,"rows_kept":47,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXB-B"]
[]
[]
[]
[]
["","","","","FTXB25B1V1","FTXB25BV1","FTXB35BV1","FTXB35B1V1","FTXB50BV1B","FTXB60BV1B"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","38","38","40","40","40","43"]
["","","Mittel","dB(A)","33","","","34"]
["","","Flüsterbetrieb","dB(A)","25","25","23","23","32","33"]
["","","Niedrig","dB(A)","28","28","26","26","35","37"]
["","Kühlung","Medium","dB(A)","33","","","34"]
["","","Flüsterbetrieb","dB(A)","22","22","25","25","32","33"]
["","","Besonders hoch","dB(A)","","","","","44","46"]
["","","Niedrig","dB(A)","25","25","26","26","35","37"]
["","","Hoch","dB(A)","38","38","39","39","40","43"]
["","","Nom.","dB(A)","33","33","34","34","38","41"]
["","Kühlung","Nom.","dB(A)","33","33","34","34","38","41"]
["Standardzubehör","Installationsanleitung","","","1","1","1","1"]
["","Bedienungsanleitung","","","1","1","1","1"]
["","Infrarotfernbedienung","","","1","","","1"]
["","Trockenbatterien, Typ AA","","","2","","","2"]
["","Fernbedienungshalterung","","","1","1","1","1"]
["","Montageplatte","","","1","1","1","1"]
["","Befestigungsschrauben für Hauptgerät","","","2","2","2","2"]
["Control systems","Infrared remote control","","","ARC470A1","ARC470A1","ARC470A1","ARC470A1","APGS02","APGS02"]
["Piping connections","Liquid","OD","mm","6.35","6.35","6.35","6.35"]
["","Gas","AD","mm","9.5","9.5","9.5","9.5"]
["","Drain","","","18","18","18","18"]
["Leistungsaufnahme","Kühlung","Nom.","kW","0.030","0.040","0.040","0.030"]
["","Heizen","Nom.","kW","0.040","0.040","0.040","0.040"]
["Schallleistungspegel","Kühlung","","dB(A)","52","52","53","53","55","61"]
["","Heizen","","dB(A)","52","52","54","54"]
["Abmessungen","Gerät","Breite","mm","770","770","770","770","1,065","1,065"]
["","","Tiefe","mm","216","216","216","216","224","224"]
["","","Höhe","mm","283","283","283","283","310","310"]
["Casing","Colour","","","","","","","Weiß","Weiß"]
["Gewicht","Maßeinheit","","kg","7","8","8","7","14","14"]
["Spannungsversorgung","Phase","","","1~","1~","1~","1~","1~","1~"]
["","Frequenz","","Hz","50","50","50","50","50","50"]
["","Name","","","V1","V1","V1","V1","V1","V1"]
["","Spannung","","V","220-240","220-240","220-240","220-240","220-240","220-240"]
["Hinweise","","","","(1) - Enthält fluorierte Treibhausgase","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - SL: Die flüsterleise Ventilatorstufe der Luftmengeneinstellung.","(1) - Enthält fluorierte Treibhausgase"]
["Standardzubehör","Infrarot-Fernbedienung","","","","1","1"]
["","Batterien","","","","2","2"]
["","Fotokatalytischer Luftreinigungsfilter mit Titanapatit","","","","2","2"]
["Hinweise","","","","","","","","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal).","(1) - Alle Geräte sind getestet und entsprechen ISO 5151 (Gerät ohne Kanal) oder ISO 13253 (Gerät mit Kanal)."]
["","","","","","","","","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten.","(2) - Änderungen aller Technischen Daten durch den Hersteller ohne Ankündigung vorbehalten."]