{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Schalldruckpegel","Heizen","Hoch","dB(A)","39","40"]
["","","Mittel","dB(A)","34","34"]
["","","Flüsterbetrieb","dB(A)","21","21"]
["","","Niedrig","dB(A)","28","28"]
["","Kühlung","Mittel","dB(A)","33","33"]
["","","Flüsterbetrieb","dB(A)","20","20"]
["","","Niedrig","dB(A)","25","26"]
["","","Hoch","dB(A)","39","40"]
["Standardzubehör","Installationsanleitung","","","1","1"]
["","Bedienungsanleitung","","","1","1"]
["","Infrarot-Fernbedienung","","","1","1"]
["","Trockenbatterien, Typ AAA","","","2","2"]
["","Fernbedienungshalterung","","","1","1"]
["","Montageplatte","","","1","1"]
["","Befestigungsschrauben für Hauptgerät","","","2","2"]
["Regelungssysteme","Verkabelte Fernbedienung","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Rohrleitungsanschlüsse","Flüssigkeit","AD","mm","6.35","6.35"]
["","Gas","AD","mm","9.50","9.50"]
["","Ableitung","","","18","18"]
["Leistungsaufnahme","Kühlung","Nom.","kW","0.017","0.019"]
["","Heizen","Nom.","kW","0.020","0.020"]
["Schallleistungspegel","Kühlung","","dB(A)","55","55"]
["","Heizen","","dB(A)","55","55"]
["Abmessungen","Maßeinheit","Breite","mm","770","770"]
["","","Tiefe","mm","225","225"]
["","","Höhe","mm","286","286"]
["Gehäuse","Farbe","","","Weiß","Weiß"]
["Gewicht","Maßeinheit","","kg","8.50","8.50"]
["Power supply","Phase","","","1~","1~"]
["","Frequenz","","Hz","50","50"]
["","Spannung","","V","220-240","220-240"]